6/16/2024

Vrishab Kakade

Weather Station

Build Document

Table of Contents

[📝Document Control 5](#_Toc169463282)

[📇 Introduction 6](#_Toc169463283)

[💫Project Outline: 6](#_Toc169463284)

[🤔Future Enhancements: 6](#_Toc169463285)

[✏️Data Accessibility: 6](#_Toc169463286)

[🎯Motivation: 6](#_Toc169463287)

[🧪Implementation: 6](#_Toc169463288)

[💻Hardware Setup: 7](#_Toc169463289)

[🔳 Software Setup: 7](#_Toc169463290)

[💻 Hardware Used 8](#_Toc169463291)

[🔳 Softwares 12](#_Toc169463292)

[🔗References 13](#_Toc169463293)

[🤖 Setup the Raspberry Pi 14](#_Toc169463294)

[💿Flashing the Image 14](#_Toc169463295)

[🖥️Configure the OS 22](#_Toc169463296)

[🔳 Check for Updates 22](#_Toc169463297)

[🔑Setup Private/Public Key for passwordless login 22](#_Toc169463298)

[🛠️Configure the Pi to enable certain options 22](#_Toc169463299)

[🌡️ Setup the Weather Station 27](#_Toc169463300)

[🎐 Setup the Weather Meter 27](#_Toc169463301)

[💻Hardware Overview 27](#_Toc169463302)

[🧑‍🏭Hardware Assembly 32](#_Toc169463303)

[🔳 Setup the software code (Program) 42](#_Toc169463304)

[Install Weewx 46](#_Toc169463305)

[👩‍🔧Raspberry Pi driver for Weewx 49](#_Toc169463306)

[CUSTOMIZATION 50](#_Toc169463307)

[🖥️Setup the Virtual Private Server (VPS) 54](#_Toc169463308)

[🕸️ Setup The VPS Server to act as Webserver 54](#_Toc169463309)

[🧑Create Username 54](#_Toc169463310)

[🔳 Change the default shell of weex to bash 54](#_Toc169463311)

[🔳 CHANGE SHELL COLOR FOR WEEWX TO GREEN 55](#_Toc169463312)

[🔳 CHANGE SHELL COLOR FOR ROOT TO RED 55](#_Toc169463313)

[🔑 SETUP KEYPAIR FOR WEEWX TO LOGIN WITHOUT A PASSWORD. 56](#_Toc169463314)

[🦾Add weewx to sudo 65](#_Toc169463315)

[🕸️Install Apache Web Server 66](#_Toc169463316)

[🕸️Step 1 — Installing Apache 66](#_Toc169463317)

[🧱Step 2 — Adjusting the Firewall 66](#_Toc169463318)

[🖥️Step 3 — Checking your Web Server 67](#_Toc169463319)

[👨‍💼Step 4 — Managing the Apache Process 68](#_Toc169463320)

[💻Setup the domain name to point to the server 69](#_Toc169463321)

[🖥️Step 5 — Setting Up Virtual Hosts (Recommended) 70](#_Toc169463322)

[🗃️Step 6 – Getting Familiar with Important Apache Files and Directories 73](#_Toc169463323)

[💭 Setup the weather station to display data to the internet 74](#_Toc169463324)

[🔁Setup Rsync from Weewx to Webserver 74](#_Toc169463325)

[🔐Setup passwordless SSH 75](#_Toc169463326)

[🔛ENABLE RSYNC 77](#_Toc169463327)

[🔐Add SSL to the webserver 79](#_Toc169463328)

[❗Prerequisite 79](#_Toc169463329)

[🎖️Step 1 — Installing Certbot 79](#_Toc169463330)

[🖥️Step 2 — Checking your Apache Virtual Host Configuration 80](#_Toc169463331)

[🔐Step 4 — Obtaining an SSL Certificate 80](#_Toc169463332)

[🎖️Step 5 — Verifying Certbot Auto-Renewal 83](#_Toc169463333)

[📱Setup Android App 84](#_Toc169463334)

[➕Step 1, install the Inigo extension for weeWX. 84](#_Toc169463335)

[🌝Step 2, Almanac (optional) 84](#_Toc169463336)

[🔂Step 3, Restarting weeWX 84](#_Toc169463337)

[📃Step 4, create inigo-settings.txt 85](#_Toc169463338)

[☔Step 5, using offset rain times (optional) 85](#_Toc169463339)

[📱Step 6, installing the app 86](#_Toc169463340)

[🧘‍♂️Setup Belchertown Skin 87](#_Toc169463341)

[🌧️AerisWeather Forecast API (optional) 87](#_Toc169463342)

[📃Install Weewx-Belchertown Skin 89](#_Toc169463343)

[💿 Setup SMB Server on the Raspberry Pi 92](#_Toc169463344)

[🪈 MQTT and MQTT Websockets (optional) 93](#_Toc169463345)

[**vince** 100](#_Toc169463346)

[Windy 103](#_Toc169463347)

[**Backup¶** 105](#_Toc169463348)

# 📝Document Control

|  |  |  |
| --- | --- | --- |
| **Date** | **Version** | **Change** |
| June 16, 2024 | 1 | Initial build - The breadboard version that is used for a proof of concept |

# 📇 Introduction

## 💫Project Outline:

I'm constructing a personalised weather station to measure various atmospheric and environmental parameters. The station will monitor and display:

1. Temperature
2. Humidity
3. Barometric Pressure
4. Wind Speed
5. Wind Direction
6. Rainfall
7. Dew Point

## 🤔Future Enhancements:

1. Air Quality Index
2. UV Index
3. Light Intensity
4. Soil Moisture

## ✏️Data Accessibility:

The system will publish real-time weather data to one or many websites, allowing remote monitoring of current weather conditions.

## 🎯Motivation:

Accurate weather forecasting is crucial, particularly for farmers who rely on timely information for agricultural decision-making. Existing forecasts often cover broad regions and may not accurately reflect local conditions. By gathering localized weather data, farmers can make informed decisions regarding crop protection, fertilization, and irrigation.

## 🧪Implementation:

💻Hardware Setup: Raspberry Pi Pico microcomputer interfaced with various sensors.

🔳 Software Setup: Data storage will be managed using the Weewx platform, while data visualization will be achieved through customizable skins.

As for the weather predictions goes – the most important is the rainfall data. Ideally, I should be able to pass the captured data to Google’s Graphcast or any other AI and get a weather forecast for my specific location. The problem with weather forecasts today is that it is given for a much wider region and they might not necessarily apply to our location. For example, in the coffee estates, it would have rained a few kilometres away, but not in that estate. More accurate weather predictions for a particular region will be able to help farmers determine things like when to spray their plants, manure them and irrigate them. Regarding weather forecasts, the rainfall data is of utmost importance. Ideally, the captured data should be compatible with AI platforms like Google's Graphcast, enabling us to obtain weather forecasts specific to our location. The current challenge with weather forecasts is that they are often provided for broader regions, which may not accurately represent local conditions. In agricultural settings, for instance, rainfall can vary significantly within a few kilometers, impacting farming activities such as spraying plants, applying manure, and irrigation. Accurate and localized weather predictions for a particular region can assist farmers in making informed decisions about their crops.

## 💻 Hardware Used

I have used the below components to build the weather station v1

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sl No** | **Image** | **Part** | **From** | **Purpose** | **Qty** | **Cost** |
| 1 |  | [Raspberry Pi Zero 2 W × 1](https://robocraze.com/products/raspberry-pi-zero-2-w?_pos=1&_sid=06ae20c70&_ss=r) | Robocraze | Central Processing Unit to connect sensors and run the software | 1 | ₹ 1,649 |
| 2 |  | [Aluminum Heat Sink for Raspberry Pi Zero 2W × 1](https://robocraze.com/products/aluminum-heatsink-for-raspberry-pi-zero-2w) | Robocraze | Cooling for Raspberry Pi processor | 1 | ₹ 12 |
| 3 |  | [40x2 Pin 2.54mm Pitch Male Berg Strip × 5](https://robocraze.com/products/40x2-pin-2-54mm-pitch-male-berg-strip?_pos=6&_sid=587f4c02f&_ss=r) | Robocraze | For the Raspberry Pi GPIO (Zero doesn't come with it) | 2 | ₹ 45 |
| 4 |  | [40x2 Female Berg Strip × 5](https://robocraze.com/products/40x2-female-berg-strip) | Robocraze | For Adafruit Hat to go on top of the Pi GPIO | 2 | ₹ 100 |
| 5 |  | [530 PCS Heat Shrink Tube Wire Insulation Sleeve × 1](https://robocraze.com/products/aluminum-heatsink-for-raspberry-pi-zero-2w) | Robocraze | To seal wire joints | 1 | ₹ 354 |
| 6 |  | [5V 3A ERD Power Adapter with Micro USB cable × 1](https://robocraze.com/products/5v-3a-erd-power-adapter?_pos=18&_sid=d1751e01c&_ss=r) | Robocraze | Power suppy for the Raspberry Pi | 1 | ₹ 299 |
| 7 |  | [16 Pin Narrow IC Base - Pack of 5 × 1](https://robocraze.com/products/16-pin-narrow-ic-base?_pos=1&_sid=86f70f0b9&_ss=r) | Robocraze | For the MCP3008 analog-to-digital converter. This will be soldered to the board and the chip is replaceable. | 1 | ₹ 32 |
| 8 |  | [BME280 Temperature Sensor Module × 1](https://robocraze.com/products/bme280-temperature-sensor-module?_pos=1&_psq=bme280&_ss=e&_v=1.0) | Robocraze | Measures temperature, humidity and atmospheric pressure | 1 | ₹ 409 |
| 9 |  | [DS18B20 Waterproof Digital Thermometer Sensor Probe × 1](https://robocraze.com/products/ds18b20-waterproof-digital-thermometer-sensor-probe?_pos=45&_sid=4c2d7e00f&_ss=r) | Robocraze | Measures the ground temperature | 1 | ₹ 61 |
| 10 |  | [Solder Wire (45gm) × 1](https://robocraze.com/products/solder-wire-50gm?_pos=8&_sid=4c2d7e00f&_ss=r) | Robocraze | To solder thicker wire | 1 | ₹ 80 |
| 11 |  | [Solder Wire-1 Meter (10gm) × 1](https://robocraze.com/products/soldering-wire10gm?_pos=7&_sid=4c2d7e00f&_ss=r) | Robocraze | Thinner wire to solder | 1 | ₹ 15 |
| 12 | MCP3008 8-Channel 10-Bit A/D Converter with SPI Interface IC DIP-16 Package | [MCP3008 8-Channel 10-Bit A/D Converter with SPI Interface IC DIP-16 Package](https://www.electronicscomp.com/mcp3008-8-channel-10-bit-a-d-converter-with-spi-interface-ic-dip-16-package?search=MCP3008%208-Channel%2010-Bit%20A%2FD%20Converter%20with%20SPI%20Interface%20IC%20DIP-16%20Package) | Electronics Comp | Convert analog to digital as Raspberry Pi can only read digital signal | 1 | ₹ 399 |
| 13 |  | [Single Strand Hookup Wire - 22AWG (Gauge) - Yellow - 5 metre](https://www.electronicscomp.com/single-strand-hookup-wire-22awg-yellow-5metre?search=Single%20Strand%20Hookup%20Wire%20-%2022AWG%20%28Gauge%29%20-%20Yellow%20-%205%20metre) | Electronics Comp | Wires to join various components - color coded for easy identification and 22 AWG is thick enough | 2 | ₹ 35 |
| 14 | Single Strand Hookup Wire - 22AWG (Gauge) - Red - 5 metre | [Single Strand Hookup Wire - 22AWG (Gauge) - Red - 5 metre](https://www.electronicscomp.com/single-strand-hookup-wire-22awg-red-5metre?search=Single%20Strand%20Hookup%20Wire%20-%2022AWG%20%28Gauge%29%20-%20Red%20-%205%20metre) | Electronics Comp | Wires to join various components - color coded for easy identification and 22 AWG is thick enough | 2 | ₹ 35 |
| 15 | Single Strand Hookup Wire - 22AWG (Gauge) - Green - 5 metre | [Single Strand Hookup Wire - 22AWG (Gauge) - Green - 5 metre](https://www.electronicscomp.com/single-strand-hookup-wire-22awg-green-5metre?search=Single%20Strand%20Hookup%20Wire%20-%2022AWG%20%28Gauge%29%20-%20Green%20-%205%20metre) | Electronics Comp | Wires to join various components - color coded for easy identification and 22 AWG is thick enough | 2 | ₹ 35 |
| 16 | Single Strand Hookup Wire - 22AWG (Gauge) - Blue - 5 metre | [Single Strand Hookup Wire - 22AWG (Gauge) - Blue - 5 metre](https://www.electronicscomp.com/single-strand-hookup-wire-22awg-blue-5metre?search=Single%20Strand%20Hookup%20Wire%20-%2022AWG%20%28Gauge%29%20-%20Blue%20-%205%20metre) | Electronics Comp | Wires to join various components - color coded for easy identification and 22 AWG is thick enough | 2 | ₹ 35 |
| 17 | Single Strand Hookup Wire - 22AWG (Gauge) - Black - 5 metre | [Single Strand Hookup Wire - 22AWG (Gauge) - Black - 5 metre](https://www.electronicscomp.com/single-strand-hookup-wire-22awg-black-5metre?search=Single%20Strand%20Hookup%20Wire%20-%2022AWG%20%28Gauge%29%20-%20Black%20-%205%20metre) | Electronics Comp | Wires to join various components - color coded for easy identification and 22 AWG is thick enough | 2 | ₹ 35 |
| 18 |  | [Adafruit 2310 Raspberry Pi Perma Prototype Hat Development Board - No Eeprom 31AC4589 × 1](https://www.tanotis.com/products/adafruit-2310-raspberry-pi-perma-prototype-hat-development-board-no-eeprom-31ac4589?variant=12550185353301) | Tanotis | To build a HAT on top of the Raspberry Pi. Components will be soldered to this board for a stable instrument | 1 | ₹ 684 |
| 19 |  | [SparkFun RJ11 6-Pin Connector Connectors × 4](https://www.tanotis.com/products/genuine-sparkfun-rj11-6-pin-connector?variant=19059938629) | Tanotis | To connect the weather station instrument (Hard to get, so bought extra) | 4 | ₹ 543 |
| 20 | Weather Meter Kit SparkFun | [Weather Meter Kit SparkFun](https://evelta.com/weather-meter-kit-sparkfun/) | Evelta | To measure wind speed, wind direct and rainfall | 1 | ₹ 7,841 |
| 21 | RJ11 Breakout 6-Pin Connector SparkFun (1 Pair) | [RJ11 Breakout 6-Pin Connector SparkFun (1 Pair)](https://evelta.com/bob-14021-rj11-breakout-6-pin-connector-sparkfun/) | Evelta | To connect the RJ 11 telephone jacks (hard to get, so got extra) | 1 | ₹ 166 |
| 22 |  | [HASTHIP® Wire Crimping Tool Wire Cutter Ratchet Wire Crimper Set with 1550PCS Dupont Connectors Male/Female Pin 0.1-1.0mm² for 2.54/3.96mm KF2510 Connector 28-18AWG](https://www.amazon.in/gp/product/B0CJDVTLJ8/ref=ppx_od_dt_b_asin_title_s01?ie=UTF8&psc=1) | Amazon | To connect wires to dupont conenctors | 1 | ₹ 1,899 |
| 23 |  | [SanDisk Ultra 64GB microSDXC UHS-I, 140MB/s R, Memory Card, 10 Y Warranty, for Smartphones](https://www.amazon.in/gp/product/B0BDRVFDKP/ref=ppx_od_dt_b_asin_title_s01?ie=UTF8&psc=1) | Amazon | Install Raspberry Pi OS | 1 | ₹ 538 |
| 24 |  | [GLOBOMOTIVE ABS Junction Box - Waterproof Electronic Project Box Enclosure Case for Electronic Projects, Outdoor, Indoor (200 X 155 x 80 mm)](https://www.amazon.in/gp/product/B0B1QN2LSH/ref=ppx_od_dt_b_asin_title_s01?ie=UTF8&psc=1) | Amazon | Waterproof housing for the Raspberry Pi and sensors | 1 | ₹ 679 |
| 25 |  | [GLOBOMOTIVE ABS Junction Box - Waterproof Electronic Project Box Enclosure Case for Electronic Projects, Outdoor, Indoor (100 x 100 x 70 mm)](https://www.amazon.in/gp/product/B0BTMBBTNV/ref=ppx_od_dt_b_asin_title_s00?ie=UTF8&psc=1) | Amazon | Waterproof housing for the BME280 sensor | 1 | ₹ 679 |
| 26 |  | [GLOBOMOTIVE Plastic Adjustable IP68 Waterproof Cable Glands Joints (PG 13.5, 10)](https://www.amazon.in/gp/product/B09HGW559M/ref=ppx_od_dt_b_asin_title_s00?ie=UTF8&psc=1) | Amazon | To run cables in the boxes so that rats don't go in | 1 | ₹ 289 |
| 27 | 4.7K Ohm 0.5W Metal Film Resistor (Pack Of 50) | [4.7k Ohm 0.5W Metal Film Resistor (Pack of 50) × 1](https://robu.in/product/4-7k-ohm-0-5w-metal-film-resistor-pack-of-50/) | Robu | For the circuit. We will only need 2 | 1 | ₹ 35 |
| 28 | Plusivo Soldering Kit (Eu Plug) With Diagonal Wire Cutter | [Plusivo Soldering Kit With Diagonal Wire Cutter × 1](https://robu.in/product/plusivo-soldering-kit-with-diagonal-wire-cutter/) | Robu | To solder the sensors and parts to the board | 1 | ₹ 1,366 |

## 🔳 Softwares

|  |  |  |
| --- | --- | --- |
| **Software** | **Version** | **Used for** |
| [Raspberry Pi OS](https://www.raspberrypi.com/software/) | [Raspberry Pi OS Lite Release date: March 15th 2024 System: 32-bit Kernel version: 6.6 Debian version: 12 (bookworm)](https://downloads.raspberrypi.com/raspios_lite_armhf/images/raspios_lite_armhf-2024-03-15/2024-03-15-raspios-bookworm-armhf-lite.img.xz) | I'm picking a non-desktop variant as I only need this to run the weather station and nothing else and the Zero 2 W hardware isn't very powerful |
| [WeeWX](https://weewx.com/docs/5.0/) | 5 | Storing data and frontend data display |
| [Apache](https://httpd.apache.org/) | 2.4 | Web server to display the reports generated by WeeWX in a web browser |
| [WeeWX driver implementation of the Build Your Own Weather Station](https://github.com/jardiamj/BYOWS_RPi/tree/master) | 0.51 | byows\_rpi - This is an weeWX driver implementation of the Build Your Own Weather Station guide produced by the Raspberry Pi Organization |


## 🔗References

|  |  |
| --- | --- |
| **Source** | **Used For** |
| [Raspberry Pi Foundation - Build your own weather station](https://projects.raspberrypi.org/en/projects/build-your-own-weather-station/0) | Tutorial to build the weather station hardware and base software |
| [Raspberry Pi Oracle Weather Station Python Code](https://github.com/RaspberryPiFoundation/weather-station) | Starting point to write the code already written by Raspberry Pi Foundation |
| [WeeWX](https://weewx.com/docs/5.0/) | Storing data and frontend data display |
| [WeeWX Wiki](https://github.com/weewx/weewx/wiki) | Good information about WeeWX - between their base doc and this all can be found |
| [Install Apache](https://projects.raspberrypi.org/en/projects/lamp-web-server-with-wordpress/2) | Web server to display the reports generated by WeeWX in a web browser |
| [WeeWX driver implementation of the Build Your Own Weather Station](https://github.com/jardiamj/BYOWS_RPi/tree/master) | Installation of the driver |
|  |  |
| Other's blogs on how to get WeeWX to work |  |
|  |  |
| [MATTHEW PIERCEY - MAKING A CUSTOM OFFLINE WEATHER STATION WITH WEEWX](https://overscore.media/posts/making-a-custom-offline-weather-station-with-weewx) | Excellent resource to give information about other resources |
| [Nev and Gays Home Weather](https://powersolarweather.duckdns.org:8046/weather/belchertown/about/) | Another good resource for information about WeeWX |
| [Setting up MQTT Broker](https://obrienlabs.net/how-to-setup-your-own-mqtt-broker/) |  |
|  |  |
| Other's Pi stations |  |
|  |  |
| [BC Robotics Raspberry Pi Weather Station](https://bc-robotics.com/tutorials/raspberry-pi-weather-station-part-1/) | Good information to see what others have done |
| [Raspberry Pi BME280 Weather Station Using Python and Flask](https://www.youtube.com/watch?v=-JtaMrrgePw&ab_channel=DonskyTech) | [Very well documented by this guy and good instructions](https://www.donskytech.com/raspberry-pi-bme280-weather-station-using-python-and-flask/) |
| [Complete DIY Raspberry Pi Weather Station With Software](https://www.instructables.com/Complete-DIY-Raspberry-Pi-Weather-Station-with-Sof/) |  |
| [Solar Powered WiFi Weather Station V2.0](https://www.instructables.com/Solar-Powered-WiFi-Weather-Station-V20/) |  |
| [Open Weather Station](https://openweatherstation.com/ows/index.php) | Done on an Aurdino |
| [Uploading weather data to Weather Underground](https://projects.raspberrypi.org/en/projects/uploading-weather-data-to-weather-underground/0) | Upload the data to Weather Underground |

# 🤖 Setup the Raspberry Pi


## 💿Flashing the Image

1. Download and install the Raspberry Pi Imager from [Raspberry Pi OS – Raspberry Pi](https://www.raspberrypi.com/software/) for Windows




2. Insert the microSD card into the PC and launch the imager. The imager can download the required software and do the work, but in my case, I’ve downloaded the software ahead of time as I have internet restrictions at times.


Download the 32 bit Lite version software from [Operating system images – Raspberry Pi](https://www.raspberrypi.com/software/operating-systems/)




32-bit and lite version should do as I don’t need a desktop and I’m using Raspberry Pi Zero 2 W which only has 512 MB of memory. So 64 bit isn’t required and I don’t want to overhead of running GUI. I’m only going to run the weather station software on this hardware.

3. Click on choose device and select Raspberry Pi Zero 2 W







4. Next click on Choose OS -> Use custom (Select a custom .img from your computer



Select the 2024-03-15-raspios-bookworm-armhf-lite.img.xz file that was previously downloaded.



Select the storage




Click Next






Edit Settings



Enable SSH



Click Save. Say Yes to apply customization and you will see the below screen. Say Yes



Once this is complete, remove the microSD card and insert it into the Pi.

## 🖥️Configure the OS

Now the Raspberry Pi is ready to be booted up. Plug it into the power source.

Using putty or any other terminal application, login. In my case the hostname is bettaforecastpi

### 🔳 Check for Updates

weewx@bettaforecastpi:~ $ sudo apt update

weewx@bettaforecastpi:~ $ sudo apt upgrade

### 🔑Setup Private/Public Key for passwordless login

See the section “[SETUP KEYPAIR FOR WEEWX TO LOGIN WITHOUT A PASSWORD](#_🔑_SETUP_KEYPAIR)” for details on how to generate the keypair. The same steps apply here.

Once you have completed the setup, you should be able to login as weewx without any password.

### 🛠️Configure the Pi to enable certain options

I create a script with the command as I keep forgetting it.


weewx@bettaforecastpi:~/.ssh $ cd

weewx@bettaforecastpi:~ $ vi raspberry\_config.sh

sudo raspi-config

Run the command


weewx@bettaforecastpi:~ $ sudo raspi-config



Select “8 Update”

Then run the below option to enable interfaces

3 Interface Options



Enable SPI, I2C, Serial Port, 1-Wire and Remote GPIO. Click Finish once done.

weewx@bettaforecastpi:~ $ mkdir weather-station/

weewx@bettaforecastpi:~ $ cd weather-station/

weewx@bettaforecastpi:~/weather-station $ vi bme280\_sensor.py

Paste and change the address to 0x76 from 0x77

address = 0x76

weewx@bettaforecastpi:~/weather-station $ python bme280\_sensor.py

weewx@bettaforecastpi:~/weather-station $ sudo apt install python3-pip

weewx@bettaforecastpi:~/weather-station $ pip --version

pip 23.0.1 from /usr/lib/python3/dist-packages/pip (python 3.11)

weewx@bettaforecastpi:~/weather-station $ sudo pip3 install RPi.bme280

error: externally-managed-environment

× This environment is externally managed

╰─> To install Python packages system-wide, try apt install

python3-xyz, where xyz is the package you are trying to

install.

If you wish to install a non-Debian-packaged Python package,

create a virtual environment using python3 -m venv path/to/venv.

Then use path/to/venv/bin/python and path/to/venv/bin/pip. Make

sure you have python3-full installed.

For more information visit http://rptl.io/venv

note: If you believe this is a mistake, please contact your Python installation or OS distribution provider. You can override this, at the risk of breaking your Python installation or OS, by passing --break-system-packages.

hint: See PEP 668 for the detailed specification.

https://www.makeuseof.com/fix-pip-error-externally-managed-environment-linux/

weewx@bettaforecastpi:/usr/lib/python3.11 $ cd /usr/lib/python3.11

weewx@bettaforecastpi:/usr/lib/python3.11 $ sudo mv EXTERNALLY-MANAGED EXTERNALLY-MANAGED.orig

weewx@bettaforecastpi:/usr/lib/python3.11 $ cd ~/weather-station/

[Humidity and temperature | Build your own weather station | Python | Coding projects for kids and teens (raspberrypi.org)](https://projects.raspberrypi.org/en/projects/build-your-own-weather-station/2)

weewx@bettaforecastpi:~ $ sudo cp /boot/firmware/config.txt /boot/firmware/config.txt.orig

weewx@bettaforecastpi:~ $ sudo vi /boot/firmware/config.txt

* Edit it by adding the line below at the bottom:

dtoverlay=w1-gpio

weewx@bettaforecastpi:~ $ sudo cp /etc/modules /etc/modules.orig

weewx@bettaforecastpi:~ $ sudo vi /etc/modules

* Add the lines below at the bottom of the file:

w1-gpio

w1-therm

Run the programs in ~/weather-station to test each module.

# 🌡️ Setup the Weather Station

## 🎐 Setup the Weather Meter

Resource: [Weather Meter Hookup Guide - SparkFun Learn](https://learn.sparkfun.com/tutorials/weather-meter-hookup-guide)



### 💻Hardware Overview

When you receive your meters, unbox all of the components, and ensure you have all of the necessary pieces.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/WeatherMeter_Parts_included.jpg)

You should have:

* Two (2) metal tubes
* Three (3) sensors:
  + rain gauge
  + anemometer
  + wind vane
* Two (2) gear clamps
* One (1) center mount armature
* One (1) side mount armature
* One (1) bag screws/nuts
* One (1) pack plastic zip ties

All of the sensors in the weather meter kit are [passive components](https://www.allaboutcircuits.com/textbook/semiconductors/chpt-1/active-versus-passive-devices/). This means you will need a voltage source in order to measure anything with them.

Each sensor is terminated with an RJ-11 connector.

#### 🌧️Rain Gauge

The rain gauge, as you may have guessed, measures rainfall. You sould get a rain gauge that looks similar to the image below.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/RainGauge.jpg)

**[Heads up!](https://learn.sparkfun.com/tutorials/weather-meter-hookup-guide" \l "rain_gauge_level)** Depending on the version of the weather meter that you receive, the rain gauge's may look different. There may be a level bubbler and a deeper reservoir for collecting water. Don't worry, the overall functionality is the same!

[](https://cdn.sparkfun.com/assets/parts/1/4/5/3/9/15901-Weather_Meter-03.jpg)

The sensor is a [self-emptying tipping bucket collector](https://www.weathershack.com/static/ed-tipping-bucket-rain-gauge.html). This means that for each **0.011" (0.2794 mm) of rain** that falls in the sensor, the bucket will tilt, dumping the water out and closing a momentary contact.

The closure of the momentary switch can be measured using interrupt pins or a digital counter. The center conductors of the RJ-11 connector are connected to the gauge's switch.

#### 🍃Anemometer


An anemometer measures wind speed.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/Anemometer_4.jpg)


The wind moves the cups on the anemometer, which in turn, rotate a enclosed magnet. The magnet closes a reed switch on each rotation, which is reflected on the output. You can measure this on the two inner conductors of the RJ-11 connector (pins 2 and 3), using a digital counter or interrupt pins on your microcontroller. To convert this into a functional wind speed, use the conversion of **1.492 mph = 1 switch closure/second**. For those in metric land, this is **2.4 km/h**.

#### 🍃Wind Vane

The wind vane indicates the direction that the wind is blowing.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/WindVane.jpg)

While you'd think think this would be a simple thing to represent with electronic components, this is actually the most complex gauges of the three. Internally on the vane are eight switches, each with their own unique resistor.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/WindVane_Switches.JPG)

The eight switches and their respective resistors internally on the wind vane.

As the wind vane rotates, a magnet closes the reed switches, and may close two at a time due to their proximity to each other. With the use of an external resistor, a voltage divider can be created. Measuring the voltage output with an analog-to-digital converter on your microcontroller allows you to determine the direction the wind vane is pointing.

As the voltage output will depend on the value of the external resistor used, there is not one common conversion function. For an example of how to calculate this, please reference the datasheet linked in the [Resources and Going Further](https://learn.sparkfun.com/tutorials/weather-meter-hookup-guide#resources-and-going-further) for the meters.

Since the values outputted by the wind vane are are based on degrees, you can, in theory, have any value represent any direction. However, we recommend having the value at degree 0 represent North for ease of use. There are also very tiny, barely-visible direction indicators on all four sides of the wind vane. If you choose different values to indicate directions, be sure to mark then accordingly. When installing and positioning your weather meters, ensure that any direction markings are pointed in the correct orientation.

Please note that the wind vane "points" in the direction **from which the wind is blowing**.

### 🧑‍🏭Hardware Assembly

The weather meter is an easy kit to assemble -- there are only mechanical connections that need to be made.

#### 🦾Armature

To begin, find the two metal tubes, and slide them together.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/Assemble_tubes.jpg)

Next, add the armature to the top of the tube set. Make sure to line up the nub on the armature with the notch in the tube.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/Armature_attachment.jpg)


Use one of the included screws and nuts to lock it in place.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/Attach_Armature_Screw.jpg)

#### 🍃Anemometer

Next, we will mount the anemometer on one side of the armature.

The anemometer has a nub on it that matches notches in the armature. This will help secure the anemometer once attached and only allows the sensor to be mounted in one direction.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/Anemometer_alignment.jpg)

Slide the anemometer onto the armature until it locks in place.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/Anemometer_attachment.jpg)

Use an included screw and nut to lock the sensor in place (make sure these are tight).

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/Anemometer_screw_attachment.jpg)

#### 🍃Wind Vane

To attach the wind vane, you will follow the same procedure as installing the anemometer.

Line up the sensor and the armature, and push the wind vane into place.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/Wind_vane_alignment.jpg)

Once again, use a screw and nut to secure the sensor in place.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/vane_screw_attachment.jpg)

#### ☔Rain Gauge

To attach the rain gauge, we also need a secondary armature. This is used to keep the rain gauge away from the other sensors to ensure it can get an accurate measurement. If the rain gauge is mounted underneath the wind vane or the anemometer, they can block rainfall into the gauge or offset the readings due to runoff.

Attach the rain gauge armature to the metal tube using the attached screws and nuts. The two halves piece together with the metal tube in between. Once you have it located where the rain gauge will be clear of the anemometer and wind vane, tighten it into place.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/Rain_gauge_Armature_Attachment.jpg)

Once again, the rain gauge has notches to ensure it mounts snugly on the armature.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/Rain_Gauge_Alignment.jpg)

Line these up, and push the rain gauge into place.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/Rain_Gauge_Attachment.jpg)

Using one of the remaining small screws, secure the rain gauge in place.


[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/AttachingRainGauge.jpg)

The rain gauge has two tabs with holes on either side. These can be used to mount the sensor on different surfaces such as rooftops or fences as well.

#### 🛠️Wire Management

If you've gotten this far, congratulations! Now it's on to the easy part -- cable management. Luckily, this isn't nearly as difficult as [some wiring projects](https://www.reddit.com/r/cablefail/).

Unravel the wires from the anemometer and the wind vane. On the bottom side of the armature, you will see clips to hold these wires in place. Slide the wire from each sensor into those.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/Wire_Management.jpg)

Once you have both of those cables plugged in, you will notice that the anemometer cable is much shorter than the wind vane. As we mentioned in the Hardware Overview, the anemometer switch conductors are shared between the anemometer and the wind vane. You will need to plug the anemometer cable into the wind vane.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/Anemometer_plugIn_to_Vane.jpg)

Run all of the remaining wires down the metal tubes, and use the included zip ties to secure them. This will prevent wind from yanking your wires out from your associated electronics.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/ZipTies.jpg)

Success! You now have an assembled weather meter! Make sure your rain gauge is clear of the anemometer and wind vane, and didn't shift during assembly. Your weather meter will look similar to the image below.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/Angled_Assembled_Meters.jpg)

You can now mount this, attach it to various electronics, or just use it as an impromptu lightsaber in battle.

#### 💈Mount the Meter (Optional)

Now that you've got your meter assembled, you need to place it somewhere with weather! You can use the included gear clamps to help mount and secure your meter.

To show a demonstration of how to use the gear clamp, we slid a gear clamp around our meter and a piece of PVC pipe. Then tighten the gear clamp using a flat head screw driver.

[](https://cdn.sparkfun.com/assets/learn_tutorials/6/8/1/Mounting_Hardware.jpg)

Keep in mind that there are many different ways to approach this problem. You will need to find a mounting solution that works specifically for your application.

#### 🔗Resources and Going Further

Now that you've successfully got your weather meter fully assembled, it's time to incorporate it into your own project!

For more information about the weather meter, check out the resources below.

* Datasheets
  + [SEN-15901](https://cdn.sparkfun.com/assets/d/1/e/0/6/DS-15901-Weather_Meter.pdf) - Latest datasheet for the weather meters. The overall functionality is the same as SEN-08942. The only difference is the [appearance of the rain gauge](https://learn.sparkfun.com/tutorials/weather-meter-hookup-guide). If you are interested, click on this link!
  + [SEN-08942](https://cdn.sparkfun.com/assets/8/4/c/d/6/Weather_Sensor_Assembly_Updated.pdf)

## 🔳 Setup the software code (Program)

Reference: [What you will need | Build your own weather station | Python | Coding projects for kids and teens (raspberrypi.org)](https://projects.raspberrypi.org/en/projects/build-your-own-weather-station/1)

This is the code written to test the hardware without Weewx. Code tutorial is from Raspberry Pi Foundation.

*# https://projects.raspberrypi.org/en/projects/build-your-own-weather-station/5*

from gpiozero import Button

from datetime import date

import time

import math

import bme280\_sensor

import wind\_direction\_byo

import statistics

import ds18b20\_therm

import database

import datetime

radius\_cm = 9.0 *# Radius in cm of the anemometer*

wind\_interval = 5 *# How often (secs) to report speed*

wind\_count = 0 *# Count how many half rotations*

CM\_IN\_A\_KM = 100000.0 *# To convert cm to km*

SECS\_IN\_A\_HOUR = 3600

ADJUSTMENT = 1.18 *# This loss of accuracy is due to something called the anemometer factor*

store\_speeds = [] *# To calculate wind gusts*

store\_directions = [] *# To store wind directions*

interval = 300 *# interval to collect data in seconds*

BUCKET\_SIZE = 0.2794 *# For rain measurement*

rain\_count = 0 *# My custom addition. Initializing this as the program throws error without it.*

today = date.today()

*# For every half rotation add 1 count*

def spin():

global wind\_count

wind\_count = wind\_count + 1

*#print("spin" + str(wind\_count))*

*# speed = distance / time*

*# speed = (rotations \* circumference) / time*

def calculate\_speed(time\_sec):

global wind\_count

global gust

circumference\_cm = (2 \* math.pi) \* radius\_cm

rotations = wind\_count / 2.0

*# Calculate the distance travelled*

*#dist\_cm = circumference\_cm \* rotations*

dist\_km = (circumference\_cm \* rotations) / CM\_IN\_A\_KM

*#speed = dist\_cm / wind\_interval*

*#return speed*

km\_per\_sec = dist\_km / time\_sec

km\_per\_hour = km\_per\_sec \* SECS\_IN\_A\_HOUR

*# Calculate final speed*

final\_speed = km\_per\_hour \* ADJUSTMENT

return final\_speed

*# Reset wind count to 0*

def reset\_wind():

global wind\_count

wind\_count = 0

*# Reset gust count to 0*

def reset\_gust():

global gust

gust = 0

*# Rain measurement*

def bucket\_tipped():

global rain\_count

rain\_count = rain\_count + 1

*#print (rain\_count \* BUCKET\_SIZE)*

*# Reset rainfall*

def reset\_rainfall():

global rain\_count

rain\_count = 0

def report\_clock\_time():

"""Returns the current clock time in a human-readable format."""

current\_time = time.localtime()

return time.strftime("%H:%M:%S", current\_time)

wind\_speed\_sensor = Button(5)

wind\_speed\_sensor.when\_pressed = spin

temp\_probe = ds18b20\_therm.DS18B20() *# Ground temperature reading*

*# Loop through to measure wind speed and report it in 5 sec intervals*

*# This is to measure only wind speed without wind gusts*

*#while True:*

*# wind\_count = 0*

*# time.sleep(wind\_interval)*

*# print(calculate\_speed(wind\_interval), "km/h")*

rain\_sensor = Button(6)

rain\_sensor.when\_pressed = bucket\_tipped

*# Connect to the database*

db = database.weather\_database()

*# This is to measure wind gusts, wind speed and wind direction*

while True:

now = datetime.datetime.now() *# Get date and time to store timestamp in the DB*

start\_time = time.time()

while time.time() - start\_time <= interval:

wind\_start\_time = time.time()

reset\_wind()

*#time.sleep(wind\_interval)*

while time.time() - wind\_start\_time <= wind\_interval:

store\_directions.append(wind\_direction\_byo.get\_value())

final\_speed = calculate\_speed(wind\_interval) *# Add this speed to the list*

store\_speeds.append(final\_speed)

wind\_average = wind\_direction\_byo.get\_average(store\_directions)

wind\_gust = max(store\_speeds)

wind\_speed = statistics.mean(store\_speeds)

rainfall = rain\_count \* BUCKET\_SIZE

reset\_rainfall()

humidity, pressure, ambient\_temp, altitude = bme280\_sensor.read\_all()

ground\_temp = temp\_probe.read\_temp()

print("Local date and time:", today, report\_clock\_time())

print("Time:", now)

print("Average Wind Speed:", wind\_speed, "km/h")

print("Peak Wind Gust:", wind\_gust, "km/h")

print("Average Wind Direction:", wind\_average)

print("Humidity:", humidity, "%")

print("Pressure:", pressure)

print("Altitude:", altitude)

print("Ambient Temperature:", ambient\_temp, "C")

print("Ground Temperature:", ground\_temp, "C")

print("Rainfall:", rainfall, "mm")

db.insert(ambient\_temp, ground\_temp, 0, pressure, humidity, wind\_average, wind\_speed, wind\_gust, rainfall, now)

print("")

store\_speeds = []

store\_directions = []

Output:

|  |
| --- |
| Sample Output |

## Install Weewx

[Debian - WeeWX 5.0](https://weewx.com/docs/5.0/quickstarts/debian/)

Tell your system to trust weewx.com.

weewx@bettaforecastpi:~/weather-station $ sudo apt install -y wget gnupg

wget -qO - https://weewx.com/keys.html | \

sudo gpg --dearmor --output /etc/apt/trusted.gpg.d/weewx.gpg

Reading package lists... Done

Building dependency tree... Done

Reading state information... Done

wget is already the newest version (1.21.3-1+b1).

wget set to manually installed.

gnupg is already the newest version (2.2.40-1.1).

0 upgraded, 0 newly installed, 0 to remove and 1 not upgraded.

Tell **apt** where to find the WeeWX repository.

weewx@bettaforecastpi:~/weather-station $ echo "deb [arch=all] https://weewx.com/apt/python3 buster main" | \

sudo tee /etc/apt/sources.list.d/weewx.list


deb [arch=all] https://weewx.com/apt/python3 buster main


Install[**¶**](https://weewx.com/docs/5.0/quickstarts/debian/#install)


Use **apt** to install WeeWX. The installer will prompt for a location, latitude/longitude, altitude, station type, and parameters specific to your station hardware. When you are done, WeeWX will be running in the background.


**sudo apt update**


**sudo apt install weewx**

















[Install Apache.](#_🕸️Install_Apache_Web)

After installing Apache, the default page is accessible from

[Bettamugilalam, TN, IN](http://bettaforecastpi/weewx/)

You can skip the part of creating a virtual server since this will only be accessed locally and nothing else will access this site and raspberry pi. From the internet I will access the site from https://bettaforecast.in

### 👩‍🔧Raspberry Pi driver for Weewx

Source: [BYOWS\_RPi/bin/user/byows\_rpi.py at master · jardiamj/BYOWS\_RPi · GitHub](https://github.com/jardiamj/BYOWS_RPi/blob/master/bin/user/byows_rpi.py)

[BYOWS\_RPi/README.md at master · jardiamj/BYOWS\_RPi (github.com)](https://github.com/jardiamj/BYOWS_RPi/blob/master/README.md)

We will need this driver to run the hardware built with Weewx

#### Installation

download the latest release (v0.51) from GitHub into your WeeWx directory

wget https:*//github.com/ddjlabs/BYOWS\_RPi/archive/refs/tags/v0.51.zip*

Once it is downloaded, run the WeeWX Extension installer. This will install the driver and add the default configuration items to your WeeWX.conf file

sudo weectl extension install v0.51.zip

#### Configuration

To enable the byows\_rpi driver modify the weewx.conf file and change the "station\_type" variable to "BYOWS" in the "[Station]" section. Configure the driver by looking for the BYOWS stanza at the end of the file.

weewx@bettaforecastpi:~ $ cd /etc/weewx/

weewx@bettaforecastpi:/etc/weewx $ sudo vi weewx.conf

If you are using different hardware or connecting them to a different pin or port, you are able to add additional variables in the "[BYOWS]" section and thereby overwriting the default values in the byows\_rpi driver.

Optional parameters configurable in the "[BYOWS]" Section:

* **loop\_interval** : How often should the driver generate packets in seconds. Default is 2.5 seconds
* **anemometer\_pin** : Pin to which anemometer is connected, the DEFAULT is pin 5.
* **rain\_bucket\_pin** : Pin to which rain bucket is connected, the DEFAULT is pin 6.
* **bme280\_port** : port for sensor bme280. The default value is 1
* **bme280\_address** : The address for sensor bme280. The default address is 0x77. CHANGE THIS TO 0x76 as one of my chip uses this
* **mcp3008\_channel** : Channel to which wind vane is connected to on MCP3008, The DEFAULT is channel 0
* **anemometer\_adjustment** : Anemometer adjustment value, the DEFAULT is 1.18
* **bucket\_size** : Bucket Size in mm, the DEFAULT is 0.2794 mm.
* **anemometer\_radius\_cm** : Anemometer radius in cm, the DEFAULT is 9.0 cm.

## CUSTOMIZATION

Disable soil sensor data as there is an issue with it

weewx@bettaforecastpi:/etc/weewx $ cd bin/user/\

weewx@bettaforecastpi:/etc/weewx/bin/user $ sudo cp byows\_rpi.py byows\_rpi.py.orig

weewx@bettaforecastpi:/etc/weewx/bin/user $ sudo vi byows\_rpi.py

Commented out a bunch of lines

weewx@bettaforecastpi:/etc/weewx/bin/user $ sudo systemctl restart weewx

ISSUE

May 09 18:36:39 bettaforecastpi weewxd[2399]: INFO user.byows\_rpi: using driver BYOWS

May 09 18:36:39 bettaforecastpi weewxd[2399]: INFO user.byows\_rpi: driver version is 0.51

May 09 18:36:39 bettaforecastpi weewxd[2399]: 2024-05-09 18:36:39 xCreatePipe: Can't set permissions (436) for //.lgd-nfy0, No such file or direc>

May 09 18:36:39 bettaforecastpi weewxd[2399]: /usr/lib/python3/dist-packages/gpiozero/devices.py:295: PinFactoryFallback: Falling back from lgpio>

May 09 18:36:39 bettaforecastpi weewxd[2399]: warnings.warn(

May 09 18:36:39 bettaforecastpi weewxd[2399]: ERROR weewx.engine: Import of driver failed: Failed to add edge detection (<class 'RuntimeError'>)

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* Traceback (most recent call last):

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* File "/usr/share/weewx/weewx/engine.py", line 115, in setupStati>

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* self.console = loader\_function(config\_dict, self)

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* File "/etc/weewx/bin/user/byows\_rpi.py", line 44, in loader

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* return ByowsRpi(\*\*config\_dict[DRIVER\_NAME])

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* File "/etc/weewx/bin/user/byows\_rpi.py", line 72, in \_\_init\_\_

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* self.station = ByowsRpiStation(\*\*params)

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* ^^^^^^^^^^^^^^^^^^^^^^^^^

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* File "/etc/weewx/bin/user/byows\_rpi.py", line 103, in \_\_init\_\_

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* self.wind\_gauge = WindGauge(

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* ^^^^^^^^^^

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* File "/etc/weewx/bin/user/byows\_rpi.py", line 238, in \_\_init\_\_

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* self.wind\_speed\_sensor = Button(anem\_pin)

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* ^^^^^^^^^^^^^^^^

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* File "/usr/lib/python3/dist-packages/gpiozero/devices.py", line >

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* self = super().\_\_call\_\_(\*args, \*\*kwargs)

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* File "/usr/lib/python3/dist-packages/gpiozero/input\_devices.py",>

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* super().\_\_init\_\_(

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* File "/usr/lib/python3/dist-packages/gpiozero/mixins.py", line 4>

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* super().\_\_init\_\_(\*args, \*\*kwargs)

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* File "/usr/lib/python3/dist-packages/gpiozero/input\_devices.py",>

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* self.pin.when\_changed = self.\_pin\_changed

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* ^^^^^^^^^^^^^^^^^^^^^

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* File "/usr/lib/python3/dist-packages/gpiozero/pins/\_\_init\_\_.py",>

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* lambda self, value: self.\_set\_when\_changed(value),

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* File "/usr/lib/python3/dist-packages/gpiozero/pins/pi.py", line >

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* self.\_enable\_event\_detect()

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* File "/usr/lib/python3/dist-packages/gpiozero/pins/rpigpio.py", >

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* GPIO.add\_event\_detect(

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL weewx.engine: \*\*\*\* RuntimeError: Failed to add edge detection

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL \_\_main\_\_: Unable to load driver: Failed to add edge detection

May 09 18:36:39 bettaforecastpi weewxd[2399]: CRITICAL \_\_main\_\_: \*\*\*\* Exiting...

May 09 18:36:40 bettaforecastpi systemd[1]: weewx.service: Main process exited, code=exited, status=4/NOPERMISSION

May 09 18:36:40 bettaforecastpi systemd[1]: weewx.service: Failed with result 'exit-code'.

weewx@bettaforecastpi:/etc/weewx/bin/user $ sudo cp /lib/systemd/system/weewx.service /lib/systemd/system/weewx.service.orig

weewx@bettaforecastpi:/etc/weewx/bin/user $ sudo vi /lib/systemd/system/weewx.service

Comment

#User=weewx

#Group=weewx

weewx@bettaforecastpi:/etc/weewx/bin/user $ sudo systemctl daemon-reload

weewx@bettaforecastpi:/etc/weewx/bin/user $ sudo systemctl start weewx

weewx@bettaforecastpi:/etc/weewx/bin/user $

weewx@bettaforecastpi:/etc/weewx/bin/user $

weewx@bettaforecastpi:/etc/weewx/bin/user $ sudo systemctl status weewx

Run reports manually

weewx@bettaforecastpi:/var/www/html/weewx $ sudo weectl report run

# 🖥️Setup the Virtual Private Server (VPS)

## 🕸️ Setup The VPS Server to act as Webserver

I have procured a VPS from [Annai Tech](https://portal.annaitech.in/). I will use this to act as the webserver to display the front end.

Server Public IP: 142.171.13.19

Hostname: cloud009.annaiservers.com

DISTRIB\_ID: Ubuntu

DISTRIB\_RELEASE: 22.04

### 🧑Create Username

Create a username called weewx that we will use to install the web server

Source: [How to Create Users in Linux (useradd Command) | Linuxize](https://linuxize.com/post/how-to-create-users-in-linux-using-the-useradd-command/)

root@cloud009:~# useradd weewx

root@cloud009:~# id weewx

uid=1000(**weewx**) gid=1000(**weewx**) groups=1000(**weewx**)

Create user password

root@cloud009:~# passwd weewx

New password:  
Retype **new** password:  
passwd: password updated successfully

Since -m option wasn’t passed when creating the user, run the below command to add home directory for the weewx user

root@cloud009:~# mkhomedir\_helper weewx

### 🔳 Change the default shell of weex to bash

$ echo $SHELL

/bin/sh

$ cat /etc/shells

# /etc/shells: valid login shells  
/bin/sh  
/bin/bash  
/usr/bin/bash  
/bin/rbash  
/usr/bin/rbash  
/usr/bin/sh  
/bin/dash  
/usr/bin/dash  
/usr/bin/tmux  
/usr/bin/screen

$ chsh

Password:  
Changing the login shell **for** weewx  
Enter the new value, **or** press ENTER **for** the default  
 Login Shell [/bin/sh]: /bin/bash

$ echo $SHELL

/bin/sh

### 🔳 CHANGE SHELL COLOR FOR WEEWX TO GREEN

This will help identify if I’ve logged in as root or weewx

weewx@cloud009:~$ cp .bashrc .bashrc.orig

weewx@cloud009:~$ vi .bashrc

Add the below

export PS1="\e[0;31m[\u@\h \w]\$ \e[m"  
source ~/.bashrc

### 🔳 CHANGE SHELL COLOR FOR ROOT TO RED

root@cloud009:~# cp .bashrc .bashrc.orig

root@cloud009:~# vi .bashrc

Add the below


export PS1="\e[0;32m[\u@\h \w]\$ \e[m"  
source ~/.bashrc

Here is a reference of all the colour codes that can be used.


|  |  |
| --- | --- |
| **Color Code** | **Color** |
| 0;30 | Black |
| 0;31 | Red |
| 0;32 | Green |
| 0;33 | Brown |
| 0;34 | Blue |
| 0;35 | Purple |
| 0;36 | Cyan |
| 0;37 | White |

### 🔑 SETUP KEYPAIR FOR WEEWX TO LOGIN WITHOUT A PASSWORD.


Use Puttygen to generate the keypair



Click on “Generate”



Move your mouse randomly inside the box.



Save the public and private keys to a file in a secure location.

Copy the public key to the server.

Login as weewx


[weewx@cloud009 ~]$ cd ~

[weewx@cloud009 ~]$ mkdir .ssh


[weewx@cloud009 ~]$ cd .ssh

[weewx@cloud009 ~/.ssh]$ vi authorized\_keys


ssh-rsa AAAAB3NzaC1yc2EAAAADAQABAAABAQC1rcBQPFmyozapzfZvJEUpKIqkNTUmOwvcsD1xiAUgRSM2Xn7gJAr9WZ+lqNSEm23W5FjYxMjZl1C5quXJiIme8Y0FInyG7XqSyXtcUDoJbKuxMDJYUdnfwJNVaLTsIThx5Xzv/zXGR1BAExLPo9lTFO0ODLeKnZIrmB/tAK4hWgeR5zc1DeSaOVL/3txnIpL7d6wme/uS7InVp5UGUPtT05a207Lt8a+CVl7cGSN6SssiGCsFeodrAqrVE5Ov0PsNDZS/VrfWdTv8vVU/4x44v5/3h1D8VQiIIcAlc9ivFAkxURMtB3qHKgyfDeexAQlgc3eae+1Lbw87Kzry6Ryb rsa-key-20240411




Create a session in putty



Pass the private key file




Save



Change the title of the session to show the username and hostname

[How can I set PuTTY's window title to the name of the loaded session? - Server Fault](https://serverfault.com/questions/178469/how-can-i-set-puttys-window-title-to-the-name-of-the-loaded-session)

Test logging in

### 🦾Add weewx to sudo

Source: [How To Create A New Sudo Enabled User on Ubuntu | DigitalOcean](https://www.digitalocean.com/community/tutorials/how-to-create-a-new-sudo-enabled-user-on-ubuntu)

[weewx@cloud009 ~]$ groups

**weewx**

root@cloud009:~# usermod -aG sudo weewx

root@cloud009:~# su - weewx

To run **a** command as administrator (user "root"), use "sudo <command>".  
See "man sudo\_root" **for** **details**.

[weewx@cloud009 ~]$ groups

**weewx sudo**

## 🕸️Install Apache Web Server

Source: [How To Install the Apache Web Server on Ubuntu | DigitalOcean](https://www.digitalocean.com/community/tutorials/how-to-install-the-apache-web-server-on-ubuntu-22-04)

### 🕸️[Step 1 — Installing Apache](https://www.digitalocean.com/community/tutorials/how-to-install-the-apache-web-server-on-ubuntu-22-04#step-1-installing-apache)

Apache is available within Ubuntu’s default software repositories, making it possible to install it using conventional package management tools.

Begin by updating the local package index to reflect the latest upstream changes. Then, install the apache2 package:

[weewx@cloud009 ~]$ sudo apt update

[weewx@cloud009 ~]$ sudo apt install apache2

### 🧱[Step 2 — Adjusting the Firewall](https://www.digitalocean.com/community/tutorials/how-to-install-the-apache-web-server-on-ubuntu-22-04#step-2-adjusting-the-firewall)

Before testing Apache, it’s necessary to modify the firewall settings to allow outside access to the default web ports. If you followed the instructions in the prerequisites, you should have a UFW firewall configured to restrict access to your server.

During installation, Apache registers itself with UFW to provide a few application profiles that can be used to enable or disable access to Apache through the firewall.

List the ufw application profiles by running the following:

[weewx@cloud009 ~]$ sudo ufw app list

Available applications:  
 Apache  
 Apache Full  
 Apache Secure  
 OpenSSH

As indicated by the output, there are three profiles available for Apache:

* Apache: This profile opens only port 80 (normal, unencrypted web traffic)
* Apache Full: This profile opens both port 80 (normal, unencrypted web traffic) and port 443 (TLS/SSL encrypted traffic)
* Apache Secure: This profile opens only port 443 (TLS/SSL encrypted traffic)

Allow on HTTP and HTTPS

[weewx@cloud009 ~]$ sudo ufw allow 'Apache Full'

Rules updated  
Rules updated (**v6**)

Firewall isn’t active

[weewx@cloud009 ~]$ sudo ufw status

Status: inactive

### 🖥️[Step 3 — Checking your Web Server](https://www.digitalocean.com/community/tutorials/how-to-install-the-apache-web-server-on-ubuntu-22-04#step-3-checking-your-web-server)


At the end of the installation process, Ubuntu starts Apache. The web server will already be up and running.

Make sure the service is active by running the command for the systemd init system:

[weewx@cloud009 ~]$ sudo systemctl status apache2

● apache2.service - The Apache HTTP Server  
 Loaded: loaded (/lib/systemd/system/apache2.service; enabled; vendor preset: enabled)  
 Active: active (running) since Fri 2024-04-12 06:06:06 UTC; 3min 12s ago  
 Docs: https://httpd.apache.org/docs/2.4/  
 Main PID: 9806 (apache2)  
 Tasks: 55 (limit: 2220)  
 Memory: 5.0M  
 CPU: 59ms  
 CGroup: /system.slice/apache2.service  
 ├─9806 /usr/sbin/apache2 -k start  
 ├─9807 /usr/sbin/apache2 -k start  
 └─9808 /usr/sbin/apache2 -k start  
  
Apr 12 06:06:06 cloud009.annaiservers.com systemd[1]: Starting The Apache HTTP Server...  
Apr 12 06:06:06 cloud009.annaiservers.com apachectl[9805]: AH00558: apache2: Could **not** reliably determine the server's fully qualified domain name, using cloud009.annaiservers.>  
Apr 12 06:06:06 cloud009.annaiservers.com systemd[1]: Started The Apache HTTP Server.

Test the page <http://142.171.13.19>



### 👨‍💼[Step 4 — Managing the Apache Process](https://www.digitalocean.com/community/tutorials/how-to-install-the-apache-web-server-on-ubuntu-22-04#step-4-managing-the-apache-process)

Now that you have your web server up and running, let’s review some basic management commands using systemctl.

To stop, start and restart your web server, run:

sudo systemctl stop apache2

sudo systemctl start apache2

sudo systemctl restart apache2

If you are simply making configuration changes, Apache can often reload without dropping connections. To do this, use the following command:

sudo systemctl reload apache2

By default, Apache is configured to start automatically when the server boots. If this is not what you want, disable this behavior by running: (Next command is to enable)

sudo systemctl disable apache2

sudo systemctl enable apache2

### 💻Setup the domain name to point to the server

Source: [How to Point a Domain Name to VPS (hostinger.in)](https://www.hostinger.in/tutorials/dns/how-to-point-domain-to-vps?ppc_campaign=google_search_generic_hosting_all&bidkw=defaultkeyword&lo=9183213&gad_source=1&gclid=CjwKCAjwt-OwBhBnEiwAgwzrUi-3cF_HY1wTfmwWbqozF5o4wLp7YHXWF69k6tubTihCKGxrevHKAxoCDwQQAvD_BwE)


I have purchased a domain called bettaforecast.in from [Hostinger](https://hpanel.hostinger.com/domain/bettaforecast.in/dns)

To use a custom domain name with a [**virtual private server**](https://www.hostinger.in/vps-hosting) (VPS), you must make a few DNS changes. Otherwise, your website will become inaccessible since the DNS server can’t resolve your domain into its IP address.


In this tutorial, we’ll show you how to point a domain name to VPS using three methods – changing the A record, configuring Cloudflare, or using custom nameservers.

If you purchased the domain from Hostinger, you can easily change the DNS record entries via hPanel:

1. Navigate to**hPanel**→**Domains**and select the domain in question.
2. Click**DNS/Nameserver**on the sidebar.
3. In the **DNS record**tab, go to the **Manage DNS records** section.
4. Find an existing **A and CNAME record** type in the DNS zone and replace their value with your VPS**IP address**.



You can test by clicking on [intoDNS: bettaforecast.in - check DNS server and mail server health](https://intodns.com/bettaforecast.in)



### 🖥️[Step 5 — Setting Up Virtual Hosts (Recommended)](https://www.digitalocean.com/community/tutorials/how-to-install-the-apache-web-server-on-ubuntu-22-04#step-5-setting-up-virtual-hosts-recommended)

I’m setting up apache on a remote server to display reports.

When using the Apache web server, you can use *virtual hosts* (similar to server blocks in Nginx) to encapsulate configuration details and host more than one domain from a single server. We will set up a domain called **bettaforecast**.

Apache on Ubuntu has one server block enabled by default that is configured to serve documents from the /var/www/html directory. While this works well for a single site, it can become unwieldy if you are hosting multiple sites. Instead of modifying /var/www/html, create a directory structure within /var/www for a **bettaforecast** site, leaving /var/www/html in place as the default directory to be served if a client request doesn’t match any other sites.

The permissions of your web root should be correct if you haven’t modified your umask value, which sets default file permissions. To ensure that your permissions are correct and allow the owner to read, write, and execute the files while granting only read and execute permissions to groups and others, you can input the following command:

[weewx@cloud009 ~]$ sudo mkdir /var/www/bettaforecast

[weewx@cloud009 ~]$ sudo chown -R $USER:$USER /var/www/bettaforecast/

[weewx@cloud009 ~]$ sudo chmod -R 755 /var/www/bettaforecast/

 Next, create a sample index.html page

[weewx@cloud009 ~]$ sudo vi /var/www/bettaforecast/index.html

<**html**>  
 <**head**>  
 <**title**>Welcome to Betta Forecast!</**title**>  
 </**head**>  
 <**body**>  
 <**h1**>Success! The bettaforecast virtual host is working!</**h1**>  
 </**body**>  
</**html**>

In order for Apache to serve this content, it’s necessary to create a virtual host file with the correct directives. Instead of modifying the default configuration file located at /etc/apache2/sites-available/000-default.conf directly, make a new one at /etc/apache2/sites-available/bettaforecast.conf:

[weewx@cloud009 ~]$ sudo vi /etc/apache2/sites-available/bettaforecast.conf

<VirtualHost \*:80>  
 ServerAdmin vrishabkakade@gmail.com  
 ServerName bettaforecast.in  
 ServerAlias www.bettaforecast  
 DocumentRoot /var/www/bettaforecast  
 ErrorLog ${APACHE\_LOG\_DIR}/error.log  
 CustomLog ${APACHE\_LOG\_DIR}/access.log combined  
</VirtualHost>

Notice that we’ve updated the DocumentRoot to our new directory and ServerAdmin to an email that the **bettaforecast** site administrator can access. We’ve also added two directives: ServerName, which establishes the base domain that will match this virtual host definition, and ServerAlias, which defines further names that will match as if they were the base name.

Save and close the file when you are finished.

Now enable the file with the a2ensite tool:

[weewx@cloud009 ~]$ sudo a2ensite bettaforecbettaforecast.conf

Enabling site bettaforecast.  
**To** activate the **new** **configuration**, you need **to** run:  
 systemctl reload apache2

Disable the default site defined in 000-default.conf:

[weewx@cloud009 ~]$ sudo a2dissite 000-default.conf

Site 000-**default** disabled.  
**To** activate the **new** **configuration**, you need **to** run:  
 systemctl reload apache2

Next, test for configuration errors:

[weewx@cloud009 ~]$ sudo apache2ctl configtest

AH00558: apache2: Could **not** reliably determine the server's fully qualified domain name, using cloud009.annaiservers.com. Set the 'ServerName' directive globally to suppress this message  
Syntax OK

Restart Apache to implement your changes:

[weewx@cloud009 ~]$ sudo systemctl restart apache2

### 🗃️[Step 6 – Getting Familiar with Important Apache Files and Directories](https://www.digitalocean.com/community/tutorials/how-to-install-the-apache-web-server-on-ubuntu-22-04#step-6-getting-familiar-with-important-apache-files-and-directories)

Now that you know how to manage the Apache service itself, you should take a few minutes to familiarize yourself with a few important directories and files.

#### [Content](https://www.digitalocean.com/community/tutorials/how-to-install-the-apache-web-server-on-ubuntu-22-04#content)

* /var/www/html: The actual web content, which by default only consists of the default Apache page you saw earlier, is served out of the /var/www/html directory. This can be changed by altering Apache configuration files.

#### [Server Configuration](https://www.digitalocean.com/community/tutorials/how-to-install-the-apache-web-server-on-ubuntu-22-04#server-configuration)

* /etc/apache2: The Apache configuration directory. All of the Apache configuration files reside here.
* /etc/apache2/apache2.conf: The main Apache configuration file. This can be modified to make changes to the Apache global configuration. This file is responsible for loading many of the other files in the configuration directory.
* /etc/apache2/ports.conf: This file specifies the ports that Apache will listen on. By default, Apache listens on port 80 and additionally listens on port 443 when a module providing SSL capabilities is enabled.
* /etc/apache2/sites-available/: The directory where per-site virtual hosts can be stored. Apache will not use the configuration files found in this directory unless they are linked to the sites-enabled directory. Typically, all server block configuration is done in this directory and then enabled by linking to the other directory with the a2ensite command.
* /etc/apache2/sites-enabled/: The directory where enabled per-site virtual hosts are stored. Typically, these are created by linking to configuration files found in the sites-available directory with the a2ensite. Apache reads the configuration files and links found in this directory when it starts or reloads to compile a complete configuration.
* /etc/apache2/conf-available/, /etc/apache2/conf-enabled/: These directories have the same relationship as the sites-available and sites-enabled directories but are used to store configuration fragments that do not belong in a virtual host. Files in the conf-available directory can be enabled with the a2enconf command and disabled with the a2disconf command.
* /etc/apache2/mods-available/, /etc/apache2/mods-enabled/: These directories contain the available and enabled modules, respectively. Files ending in .load contain fragments to load specific modules, while files ending in .conf contain the configuration for those modules. Modules can be enabled and disabled using the a2enmod and a2dismod commands.

#### [Server Logs](https://www.digitalocean.com/community/tutorials/how-to-install-the-apache-web-server-on-ubuntu-22-04#server-logs)

* /var/log/apache2/access.log: By default, every request to your web server is recorded in this log file unless Apache is configured to do otherwise.
* /var/log/apache2/error.log: By default, all errors are recorded in this file. The LogLevel directive in the Apache configuration specifies how much detail the error logs will contain.

# 💭 Setup the weather station to display data to the internet

So far the weather station has only been accessible from the LAN. Now it is time to setup the connectivity to the webserver we created int eh previous section.

## 🔁Setup Rsync from Weewx to Webserver

Source: [[StdReport] - WeeWX 5.0](https://weewx.com/docs/5.0/reference/weewx-options/stdreport/#ciphers)

While this "report" does not actually generate anything, it uses the report machinery to upload files from directory **HTML\_ROOT** to a remote webserver using [rsync](https://rsync.samba.org/). Fast, efficient, and secure, it does an incremental update, that is, it only synchronizes those parts of a file that have changed, saving the outgoing bandwidth of your Internet connection.

If you wish to use rsync, you must configure passwordless ssh using public/private key authentication from the user account that WeeWX runs, to the user account on the remote machine where the files will be copied.

**enable**

Set to **true** (the default) to enable rsync. Set to **false** to disable.

**server**

Set to the name of your server. This name should appear in your **.ssh/config** file. Required. No default

**user**

Set to the ssh username you use for your rsync connection to your web server. The local user that WeeWX runs as must have [passwordless ssh](https://www.tecmint.com/ssh-passwordless-login-using-ssh-keygen-in-5-easy-steps/) configured for *user@server*. Required. No default.

**path**

Set to the path where the weather data will be stored on your webserver (*e.g.*, **/var/www/html/weather**). Make sure **user** has write privileges in this directory. Required. No default.

**port**

The port to use for the ssh connection. Default is to use the default port for the **ssh** command (generally 22).

**delete**

Files that don't exist in the local report are removed from the remote location.

**Warning**

USE WITH CAUTION! If you make a mistake in setting the path, this can cause unexpected files to be deleted on the remote server.

Valid values are **1** to enable and **0** to disable. Required. Default is **0**.

### 🔐Setup passwordless SSH

The weather station Raspberry Pi needs to login without a password to the webserver. I will set it up for root as I run Weewx as root. I couldn’t get it to run as non-root user even though it is supported.

vrishabkakade@freedompi.local:~/.ssh$ sudo su

root@freedompi:/home/vrishabkakade/.ssh*# cd ~*

root@freedompi:~# ls -lrat

total 40  
-rw-r--r-- 1 root root 161 Jul 9 2019 .profile  
-rw-r--r-- 1 root root 571 Apr 11 2021 .bashrc  
drwx------ 2 root root 4096 Mar 15 20:29 .ssh  
drwx------ 3 root root 4096 Mar 15 20:47 .vnc  
drwx------ 3 root root 4096 Apr 1 19:20 .cache  
-rw------- 1 root root 2143 Apr 4 21:01 .mysql\_history  
-rw-r--r-- 1 root root 180 Apr 5 18:42 .wget-hsts  
drwxr-xr-x 18 root root 4096 Apr 9 20:48 ..  
-rw------- 1 root root 20 Apr 9 20:48 .lesshst  
drwx------ 5 root root 4096 Apr 9 20:48 .

root@freedompi:~# cd .ssh

root@freedompi:~/.ssh*# vi config*

Host bettaforecat.**in**  
 HostName bettaforecast.**in**  
 User weewx  
 IdentityFile ~/.ssh/id\_rsa

root@freedompi:~/.ssh# chmod 600 ~/.ssh/config

root@freedompi:~/.ssh*# ssh-keygen*

Generating public/private rsa key pair.  
Enter file in which to save the key (/root/.ssh/id\_rsa):   
Enter passphrase (empty for no passphrase):   
Enter same passphrase again:   
Your identification has been saved in /root/.ssh/id\_rsa  
Your public key has been saved in /root/.ssh/id\_rsa.pub  
The key fingerprint is:  
SHA256:tUODf2772BiR3/luvX5I5Y10aDxv2eaQqFlwdu5HzLw root@freedompi  
The key's randomart image is:  
+---[RSA 3072]----+  
| |  
| . |  
| . + . . |  
| +.oo.B o|  
| S +++\* %+|  
| +oo\*o&|  
| ++o.O+|  
| o. \*oEB|  
| +.+\*=|  
+----[SHA256]-----+

Login to bettaforecast.in

On remote server, add the public key

[weewx@cloud009 /var/www/bettaforecast]$ cd

[weewx@cloud009 ~]$ cd .ssh/

[weewx@cloud009 ~/.ssh]$ vi authorized\_keys

ssh-rsa  root@freedompi

### 🔛ENABLE RSYNC

Back on the Raspberry Pi

vrishabkakade@freedompi:~ $ cd /etc/weewx/

vrishabkakade@freedompi:/etc/weewx $ cp weewx.conf weewx.conf.`date +%Y%m%d`

Under [StdReport]  
  
 [[RSYNC]]  
 # rsync'ing to a webserver is treated as just another report.  
 skin = Rsync  
  
 # If you wish to use rsync, you must configure passwordless ssh using  
 # public/private key authentication from the user account that weewx  
 # runs to the user account on the remote machine where the files  
 # will be copied.  
 #  
 # If you wish to use rsync, set "enable" to "true", then  
 # fill out server, user, and path.  
 # The server should appear in your .ssh/config file.  
 # The user is the username used in the identity file.  
 # The path is the destination directory, such as /var/www/html/weather.  
 # Be sure that the user has write permissions on the destination!  
 enable = true  
 server = bettaforecast.**in**  
 user = weewx  
 path = /var/www/bettaforecast  
  
 # To upload files from something other than what HTML\_ROOT is set  
 # to above, specify a different HTML\_ROOT here.  
 #HTML\_ROOT = /var/www/html/weewx  
  
 # Rsync can be configured to remove files from the remote server if  
 # they don't exist under HTML\_ROOT locally. USE WITH CAUTION: if you  
 # make a mistake in the remote path, you could could unintentionally  
 # cause unrelated files to be deleted. Set to 1 to enable remote file  
 # deletion, zero to allow files to accumulate remotely.  
 delete = 0

vrishabkakade@freedompi:/etc/weewx $ sudo systemctl restart weewx

vrishabkakade@freedompi:/etc/weewx $ sudo systemctl status weewx

● weewx.service - WeeWX  
 Loaded: loaded (/lib/systemd/system/weewx.service; enabled; preset: enabled)  
 Active: active (running) since Fri 2024-04-12 16:09:48 IST; 5s ago  
 Docs: https://weewx.com/docs  
 Main PID: 16834 (python3)  
 Tasks: 10 (limit: 4444)  
 CPU: 470ms  
 CGroup: /system.slice/weewx.service  
 └─16834 python3 /usr/share/weewx/weewxd.py /etc/weewx/weewx.conf  
  
Apr 12 16:09:48 freedompi weewxd[16834]: INFO weewx.restx: WOW: Data **for** station 00ef03c0-7cf6-ee11-a81c-0022489bcb24 will be posted  
Apr 12 16:09:48 freedompi weewxd[16834]: INFO weewx.restx: AWEKAS: Posting **not** enabled.  
Apr 12 16:09:48 freedompi weewxd[16834]: INFO user.windy: version **is** 0.7  
Apr 12 16:09:48 freedompi weewxd[16834]: INFO user.windy: Data will be uploaded to https://stations.windy.com/pws/update  
Apr 12 16:09:48 freedompi weewxd[16834]: INFO weewx.engine: 'pyephem' detected, extended almanac data **is** available  
Apr 12 16:09:48 freedompi weewxd[16834]: INFO \_\_main\_\_: Starting up weewx version 5.0.2  
Apr 12 16:09:48 freedompi weewxd[16834]: INFO weewx.engine: Using binding 'wx\_binding' to database 'weewx.sdb'  
Apr 12 16:09:48 freedompi weewxd[16834]: INFO weewx.manager: Starting backfill of daily summaries  
Apr 12 16:09:48 freedompi weewxd[16834]: INFO weewx.manager: Daily summaries up to date  
Apr 12 16:09:48 freedompi weewxd[16834]: INFO weewx.engine: Starting main packet loop.

## 🔐Add SSL to the webserver

Source: [How To Secure Apache with Let's Encrypt on Ubuntu | DigitalOcean](https://www.digitalocean.com/community/tutorials/how-to-secure-apache-with-let-s-encrypt-on-ubuntu)

Back on the webserver bettaforecast.in

Let’s Encrypt is a Certificate Authority (CA) that facilitates obtaining and installing free [TLS/SSL certificates](https://www.digitalocean.com/community/tutorials/openssl-essentials-working-with-ssl-certificates-private-keys-and-csrs), thereby enabling encrypted HTTPS on web servers. It streamlines the process by providing a software client, Certbot, that attempts to automate most (if not all) of the required steps. Currently, the entire process of obtaining and installing a certificate is fully automated on both Apache and Nginx.

In this guide, you’ll use [Certbot](https://certbot.eff.org/) to obtain a free SSL certificate for Apache on Ubuntu and make sure this certificate is set up to renew automatically.

This tutorial uses a separate virtual host file instead of Apache’s default configuration file for setting up the website that will be secured by Let’s Encrypt. [We recommend](https://www.digitalocean.com/community/tutorials/how-to-install-the-apache-web-server-on-ubuntu-22-04#step-5-setting-up-virtual-hosts-recommended) creating new Apache virtual host files for each domain hosted in a server because it helps to avoid common mistakes and maintains the default configuration files as a fallback setup.

### ❗Prerequisite

To follow this tutorial, you will need:

* One Ubuntu server set up with a non-*root* user with sudo administrative privileges and firewall enabled. You can set this up by following our [initial server setup for Ubuntu](https://www.digitalocean.com/community/tutorials/initial-server-setup-with-ubuntu) tutorial.
* A fully registered domain name. This tutorial will use **your\_domain** as an example throughout. You can purchase a domain name on [Namecheap](https://namecheap.com/), get one for free on [Freenom](http://www.freenom.com/en/index.html), or use the domain registrar of your choice.
* Both of the following DNS records set up for your server. You can follow [this introduction to DigitalOcean DNS](https://docs.digitalocean.com/products/networking/dns/) for details on how to add them.
  + An A record with your\_domain pointing to your server’s public IP address.
  + An A record with www.your\_domain pointing to your server’s public IP address.
* Apache installed by following [How To Install Apache on Ubuntu](https://www.digitalocean.com/community/tutorials/how-to-install-the-apache-web-server-on-ubuntu-22-04). Be sure that you have a [virtual host file](https://www.digitalocean.com/community/tutorials/how-to-install-the-apache-web-server-on-ubuntu-22-04#step-5-setting-up-virtual-hosts-recommended) for your domain. This tutorial will use /etc/apache2/sites-available/your\_domain.conf as an example.

### 🎖️[Step 1 — Installing Certbot](https://www.digitalocean.com/community/tutorials/how-to-secure-apache-with-let-s-encrypt-on-ubuntu" \l "step-1-installing-certbot)

To obtain an SSL certificate with Let’s Encrypt, you need to install the Certbot software on your server. You’ll use the default Ubuntu package repositories for that.

[weewx@cloud009 ~]$ sudo apt update

[weewx@cloud009 ~]$ sudo apt isudo apt install certbot python3-certbot-apache

Certbot is now installed on your server. In the next step, you’ll verify Apache’s configuration to make sure your virtual host is set appropriately. This will ensure that the certbot client script will be able to detect your domains and reconfigure your web server to use your newly generated SSL certificate automatically.

### 🖥️[Step 2 — Checking your Apache Virtual Host Configuration](https://www.digitalocean.com/community/tutorials/how-to-secure-apache-with-let-s-encrypt-on-ubuntu#step-2-checking-your-apache-virtual-host-configuration)

To automatically obtain and configure SSL for your web server, Certbot needs to find the correct virtual host within your Apache configuration files. Your server domain name(s) will be retrieved from the ServerName and ServerAlias directives defined within your VirtualHost configuration block.

If you followed the [virtual host setup step in the Apache installation tutorial](https://www.digitalocean.com/community/tutorials/how-to-install-the-apache-web-server-on-ubuntu-22-04#step-5-setting-up-virtual-hosts-recommended), you should have a VirtualHost block set up for your domain at /etc/apache2/sites-available/bettaforecast.conf with the ServerName and also the ServerAlias directives already set appropriately.

[weewx@cloud009 ~]$ sudo apache2ctl configtest

AH00558: apache2: Could **not** reliably determine the server's fully qualified domain name, using cloud009.annaiservers.com. Set the 'ServerName' directive globally to suppress this message  
Syntax OK

You should receive Syntax OK as a response. If you get an error, reopen the virtual host file and check for any typos or missing characters. Once your configuration file’s syntax is correct, reload Apache so that the changes take effect:

[weewx@cloud009 ~]$ sudo systemctl reload apache2

With these changes, Certbot will be able to find the correct VirtualHost block and update it.

Next, you’ll update the firewall to allow HTTPS traffic.

SKIP SETP 3 as no FIREWALL

### 🔐[Step 4 — Obtaining an SSL Certificate](https://www.digitalocean.com/community/tutorials/how-to-secure-apache-with-let-s-encrypt-on-ubuntu#step-4-obtaining-an-ssl-certificate)

Certbot provides a variety of ways to obtain SSL certificates through plugins. The Apache plugin will take care of reconfiguring Apache and reloading the configuration whenever necessary. To use this plugin, run the following:


[weewx@cloud009 ~]$ sudo certbot –apache

Saving debug log to /var/log/letsencrypt/letsencrypt.log  
Enter email address (used **for** urgent renewal **and** security notices)  
 (Enter 'c' to cancel): vrishabkakade@gmail.com  
  
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -  
Please read **the** Terms **of** Service **at**  
**https**://letsencrypt.org/documents/LE-SA-v1.4-April-3-2024.pdf. You must agree **in**  
order to register **with** **the** ACME server. Do you agree?  
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -  
(Y)es/(N)o: Y  
  
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -  
Would you be willing, once your **first** certificate is successfully issued, to  
share your email address **with** **the** Electronic Frontier Foundation, **a** founding  
partner **of** **the** Let's Encrypt project and the non-profit organization that  
develops Certbot? We'd like to send you email about our work encrypting **the** web,  
EFF news, campaigns, **and** ways to support digital freedom.  
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -  
(Y)es/(N)o: N  
Account registered.  
  
Which names would you like to activate HTTPS **for**?  
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -  
1: bettaforecast.**in**  
2: www.bettaforecast  
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -  
Select **the** appropriate numbers separated **by** commas **and**/**or** spaces, **or** leave input  
blank to select all options shown (Enter 'c' to cancel): 1  
Requesting **a** certificate **for** bettaforecast.**in**  
  
Successfully received certificate.  
Certificate is saved **at**: /etc/letsencrypt/live/bettaforecast.**in**/fullchain.pem  
Key is saved **at**: /etc/letsencrypt/live/bettaforecast.**in**/privkey.pem  
This certificate expires **on** **2024-07-11**.  
These files will be updated when **the** certificate renews.  
Certbot has set up **a** scheduled task to automatically renew this certificate **in** **the** background.  
  
Deploying certificate  
Successfully deployed certificate **for** bettaforecast.**in** to /etc/apache2/sites-available/bettaforecast-le-ssl.conf  
Congratulations! You have successfully enabled HTTPS **on** **https**://**bettaforecast**.**in**  
  
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -  
If you like Certbot, please consider supporting our work **by**:  
 \* Donating to ISRG / Let's Encrypt: https://letsencrypt.org/donate  
 \* Donating to EFF: https://eff.org/donate-le  
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

Your certificate is now installed and loaded into Apache’s configuration. Try reloading your website using https:// and notice your browser’s security indicator. It should indicate that your site is properly secured, typically by a lock icon in the address bar.

You can use the [SSL Labs Server Test](https://www.ssllabs.com/ssltest/) to verify your certificate’s grade and obtain detailed information about it, from the perspective of an external service.

In the next and final step, you’ll test the auto-renewal feature of Certbot, which guarantees that your certificate will be renewed automatically before the expiration date.



### 🎖️[Step 5 — Verifying Certbot Auto-Renewal](https://www.digitalocean.com/community/tutorials/how-to-secure-apache-with-let-s-encrypt-on-ubuntu#step-5-verifying-certbot-auto-renewal)

Let’s Encrypt’s certificates are only valid for ninety days. This is to encourage users to automate their certificate renewal process, as well as to ensure that misused certificates or stolen keys will expire sooner rather than later.

The certbot package you installed takes care of renewals by including a renew script to /etc/cron.d, which is managed by a systemctl service called certbot.timer. This script runs twice a day and will automatically renew any certificate that’s within thirty days of expiration.

To check the status of this service and make sure it’s active, run the following:

[weewx@cloud009 ~]$ sudo systesudo systemctl status certbot.timer

● certbot.timer - Run certbot twice daily  
 Loaded: loaded (/lib/systemd/system/certbot.timer; enabled; vendor preset: enabled)  
 Active: active (waiting) since Fri 2024-04-12 10:55:33 UTC; 11min ago  
 Trigger: Fri 2024-04-12 13:27:07 UTC; 2h 19min left  
 Triggers: ● certbot.service  
  
Apr 12 10:55:33 cloud009.annaiservers.com systemd[1]: Started Run certbot twice daily.

To test the renewal process, you can do a dry run with certbot:

[weewx@cloud009 ~]$ sudo certbot renew --dry-run

Saving debug log to /var/log/letsencrypt/letsencrypt.log  
  
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -  
Processing /etc/letsencrypt/renewal/bettaforecast.**in**.conf  
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -  
Account registered.  
Simulating renewal of an existing certificate **for** bettaforecast.**in**  
  
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -  
Congratulations, all simulated renewals succeeded:  
 /etc/letsencrypt/live/bettaforecast.**in**/fullchain.pem (success)  
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

If you don’t receive any errors, you’re all set. When necessary, Certbot will renew your certificates and reload Apache to pick up the changes. If the automated renewal process ever fails, Let’s Encrypt will send a message to the email you specified, warning you when your certificate is about to expire.

Other good docs (but not needed for my setup)

## 📱Setup Android App

Source: [Home · evilbunny2008/weeWXWeatherApp Wiki · GitHub](https://github.com/evilbunny2008/weeWXWeatherApp/wiki)

### ➕Step 1, install the Inigo extension for weeWX.

This has to be done on the Raspberry Pi as that is where Weewx is installed.

vrishabkakade@freedompi:~ $ cd /tmp

vrishabkakade@freedompi:/tmp $ wget -O inigo-metric.tar.gz https://github.com/evilbunny2008/weeWXWeatherApp/releases/download/1.0.17/inigo-metric.tar.gz

vrishabkakade@freedompi:/tmp $ sudo weectl extension install inigo-metric.tar.gz

**Using** **configuration** file /etc/weewx/weewx.conf  
Install **extension** 'inigo-metric.tar.gz' (y/n)? y  
Extracting **from** tar archive inigo-metric.tar.gz  
Saving installer file **to** /etc/weewx/bin/**user**/installer/Inigo  
Saved **copy** **of** **configuration** **as** /etc/weewx/weewx.conf.20240412182619  
Finished installing **extension** Inigo **from** inigo-metric.tar.gz

### 🌝Step 2, Almanac (optional)

If you would like to see moon rise/set in the app, you just need to install pyephem.

sudo apt -y install python3-ephem

### 🔂Step 3, Restarting weeWX

vrishabkakade@freedompi:/tmp $ sudo systemctl restart weewx

vrishabkakade@freedompi:/tmp $ sudo systemctl status weewx

● weewx.service - WeeWX  
 Loaded: loaded (/lib/systemd/system/weewx.service; enabled; preset: enabled)  
 Active: active (running) since Fri 2024-04-12 18:28:42 IST; 7s ago  
 Docs: https://weewx.com/docs  
 Main PID: 17971 (python3)  
 Tasks: 10 (limit: 4444)  
 CPU: 502ms  
 CGroup: /system.slice/weewx.service  
 └─17971 python3 /usr/share/weewx/weewxd.py /etc/weewx/weewx.conf  
  
Apr 12 18:28:43 freedompi weewxd[17971]: INFO weewx.restx: WOW: Data **for** station 00ef03c0-7cf6-ee11-a81c-0022489bcb24 will be posted  
Apr 12 18:28:43 freedompi weewxd[17971]: INFO weewx.restx: AWEKAS: Posting **not** enabled.  
Apr 12 18:28:43 freedompi weewxd[17971]: INFO user.windy: version **is** 0.7  
Apr 12 18:28:43 freedompi weewxd[17971]: INFO user.windy: Data will be uploaded to https://stations.windy.com/pws/update  
Apr 12 18:28:43 freedompi weewxd[17971]: INFO weewx.engine: 'pyephem' detected, extended almanac data **is** available  
Apr 12 18:28:43 freedompi weewxd[17971]: INFO \_\_main\_\_: Starting up weewx version 5.0.2  
Apr 12 18:28:43 freedompi weewxd[17971]: INFO weewx.engine: Using binding 'wx\_binding' to database 'weewx.sdb'  
Apr 12 18:28:43 freedompi weewxd[17971]: INFO weewx.manager: Starting backfill of daily summaries  
Apr 12 18:28:43 freedompi weewxd[17971]: INFO weewx.manager: Daily summaries up to date  
Apr 12 18:28:43 freedompi weewxd[17971]: INFO weewx.engine: Starting main packet loop.

### 📃Step 4, create inigo-settings.txt

You need to change the inigo-settings.txt to provide details about your weather stations. Full details are available [in the wiki](https://github.com/evilbunny2008/weeWXWeatherApp/wiki/InigoSettings.txt)

Once you're happy with your changes press ctrl+x to exit and save.

vrishabkakade@freedompi:/tmp $ sudo wget -O /var/www/html/weewx/inigo-settings.txt https:*//github.com/evilbunny2008/weeWXWeatherApp/releases/download/1.0.3/inigo-settings.txt*

vrishabkakade@freedompi:/tmp $ sudo vi /var/www/html/weewx/inigo-settings.txt

[weewx@cloud009 ~]$ cat /var/www/bettaforecast/inigo-settings.txt

data=https://bettaforecast.in/inigo-data.txt  
radtype=image  
radar=https://embed.windy.com/embed2.html?lat=-34&lon=151&zoom=11&level=surface&overlay=radar&menu=&message=true&marker=&calendar=&pressure=true&type=map&location=coordinates&detail=&detailLat=-34&detailLon=150&metricWind=km%2Fh&metricTemp=**%C2%B0C**&radarRange=-1  
fctype=met.no  
forecast=https://api.met.no/weatherapi/locationforecast/2.0/compact?altitude=1181&lat=12.359722&lon=77.879722  
#webcam=http://mx.cafesydney.com:8888/mjpg/video.mjpg  
#custom=http://m.bom.gov.au/nsw/sydney/radar/

### ☔Step 5, using offset rain times (optional)

Historically rainfall is measured in Australia at 9am, so it's useful for comparison reasons to be able to display rain records matching time of day with the [Bureau of Meteorology](http://www.bom.gov.au/). To enable this simply edit /etc/weewx/since.tmpl and paste the following into it:

vrishabkakade@freedompi:/etc/weewx $ vi /etc/weewx/since.tmpl

#if $varExists('since')  
$since($hour=9).rain.**sum**.formatted|$since($hour=9,$today=False).rain.**sum**.formatted|9am|#slurp  
#else  
|||#slurp  
#end **if**

### 📱Step 6, installing the app

You can now get the app from [Google Play](https://play.google.com/store/apps/details?id=com.odiousapps.weewxweather).

On first boot the app will prompt you for the URL to your inigo-settings.txt file, this is usually https://bettaforecast.in/inigo-settings.txt, once entered click save and in a few seconds you should be up and running.

Once saved the settings are cached by the app. If you need to tell the app to re-download the settings, you swipe from the left side of any screen to open the settings pane.

## 🧘‍♂️Setup Belchertown Skin

I really like this skin for all the customization options, documentation and real-time updates. In this section I will go through all the setup.

### 🌧️AerisWeather Forecast API (optional)


Source: [GitHub - poblabs/weewx-belchertown: A clean and modern weewx skin with real time streaming updates, forecast data and interactive charts. View it in action at BelchertownWeather.com](https://github.com/poblabs/weewx-belchertown#weewxconf)

AerisWeather's Forecast API is where the current observations and forecast data comes from. The skin will work without this integration, however it is used to show current weather observations and icons as well as the forecast.

**You must sign up to use their service.** This skin does not provide any forecast data. You need to join their website and get a free developer key. In order to get a free developer key, you have to send your weather data to pwsweather.com - which is an integration built into weewx. You just need to activate it! Once enabled, by default the skin will download and cache every hour.

* If you haven't already; sign up for pwsweather at <https://www.pwsweather.com/register>
* Add a new station, and configure your weewx.conf to start sending your weather data to pwsweather.
* Then sign up for a free AerisWeather developer account by linking your pwsweather account here [https://www.aerisweather.com/signup/pws](https://www.aerisweather.com/signup/pws/)
* Once you are logged in, you should make a Demo Project as part of the sign up process, then go to <https://www.aerisweather.com/account/apps> and and save these keys as forecast\_api\_id and forecast\_api\_secret.
* The rest of the options can be found below in the [Forecast Options](https://github.com/poblabs/weewx-belchertown#forecast-options) table.

GPS Location of my farm: 12.359722,77.879722



Following the instructions on the website, I obtain my key.

**❗THIS IS A SECRET. NOT TO BE SHARED.**

client\_id=IqsFS2GFixbyl8YlasOBQ  
client\_secret=zKZkQ4x6k8ipuE4ONX4phAH5PsWvxc3CtnupG3zb

Below are not required, but I just document it.

Request URL

https://data.api.xweather.com/forecasts/12.359722,77.879722?format=json&filter=day&limit=7&client\_id=IqsFS2GFixbyl8YlasOBQ&client\_secret=zKZkQ4x6k8ipuE4ONX4phAH5PsWvxc3CtnupG3zb

cURL

curl -H "Content-Type: application/json" -X GET "https://data.api.xweather.com/forecasts/12.359722, 77.879722?format=json&filter=day&limit=7&client\_id=IqsFS2GFixbyl8YlasOBQ&client\_secret=zKZkQ4x6k8ipuE4ONX4phAH5PsWvxc3CtnupG3zb"

Java Script

fetch('https://data.api.xweather.com/forecasts/12.359722, 77.879722?format=json&filter=day&limit=7&client\_id=IqsFS2GFixbyl8YlasOBQ&client\_secret=zKZkQ4x6k8ipuE4ONX4phAH5PsWvxc3CtnupG3zb')

.then((response) => {

return response.json();

})

.then((json) => {

if (!json.success) {

console.log('Oh no!');

} else {

console.log(json);

}

})

.catch((error) => {

console.log('Oh no!');

});

Python Code

import urllib

import json

request = urllib.request.urlopen('https://data.api.xweather.com/forecasts/12.359722,77.879722?format=json&filter=day&limit=7&client\_id=IqsFS2GFixbyl8YlasOBQ&client\_secret=zKZkQ4x6k8ipuE4ONX4phAH5PsWvxc3CtnupG3zb')

response = request.read()

json = json.loads(response)

if json['success']:

print(json)

else:

print("An error occurred: %s" % (json['error']['description']))

request.close()

### 📃Install Weewx-Belchertown Skin

1. Download [the latest release](https://github.com/poblabs/weewx-belchertown/releases).

vrishabkakade@freedompi:/tmp $ wget https://github.com/poblabs/weewx-belchertown/releases/download/weewx-belchertown-1.3.1/weewx-belchertown-release.1.3.1.tar.gz

vrishabkakade@freedompi:~ $ sudo weectl extension install weewx-belchertown-release.1.3.1.tar

Using **configuration** **file** /etc/weewx/weewx.conf  
Install extension 'weewx-belchertown-**release**.1.3.1.tar' (y/n)? y  
Traceback (most recent call last):  
**File** "/usr/share/weewx/weectl.py", line 74, **in**  
main()  
**File** "/usr/share/weewx/weectl.py", line 66, **in** main  
namespace.func(namespace)  
**File** "/usr/share/weewx/weectllib/init.py", line 121, **in** dispatch  
namespace.action\_func(config\_dict, namespace)  
**File** "/usr/share/weewx/weectllib/extension\_cmd.py", line 116, **in** install\_extension  
ext.install\_extension(namespace.source, no\_confirm=namespace.yes)  
**File** "/usr/share/weewx/weecfg/extension.py", line 143, **in** install\_extension  
raise InstallError(f"Unrecognized type for {extension\_path}")  
weecfg.extension.InstallError: Unrecognized **type** **for** weewx-belchertown-**release**.1.3.1.tar

v1.3.1 Threw errors constantly. So I installed 1.3

wget <https://github.com/poblabs/weewx-belchertown/releases/download/weewx-belchertown-1.3/weewx-belchertown-release-1.3.tar.gz>

vrishabkakade@freedompi:/tmp $ sudo weectl extension install weewx-belchertown-release-1.3.tar.gz

**Using** **configuration** file /etc/weewx/weewx.conf  
Install **extension** 'weewx-belchertown-release-1.3.tar.gz' (y/n)? y  
Extracting **from** tar archive weewx-belchertown-**release**-1.3.tar.gz  
Saving installer file **to** /etc/weewx/bin/**user**/installer/Belchertown  
Saved **copy** **of** **configuration** **as** /etc/weewx/weewx.conf.20240413114922  
Finished installing **extension** Belchertown **from** weewx-belchertown-**release**-1.3.tar.gz

Since I installed as sudo it changed it to root. Change permissions to weewx user

vrishabkakade@freedompi:/tmp $ cd /etc/weewx/

vrishabkakade@freedompi:/etc/weewx $ sudo chown weewx:weewx weewx.conf

vrishabkakade@freedompi:/etc/weewx $ cp weewx.conf weewx.conf.`date +%Y%m%d`

vrishabkakade@freedompi:~ $ sudo systemctl restart weewx

vrishabkakade@freedompi:~ $ sudo systemctl status weewx

I got the below error after the installation

**Uncaught** **TypeError**: **Highcharts**.chart **is** **not** **a** **constructor**  
 **at** **Object**.<**anonymous**> (**belchertown**.js?1712999116:2407:25)  
 **at** **Function**.each (**jquery**.min.js:2:2623)  
 **at** **Object**.success (**belchertown**.js?1712999116:1462:16)  
 **at** **u** (**jquery**.min.js:2:27457)  
 **at** **Object**.fireWith [as resolveWith] (**jquery**.min.js:2:28202)  
 **at** **k** (**jquery**.min.js:2:77651)  
 **at** **XMLHttpRequest**.<**anonymous**> (**jquery**.min.js:2:79907)

[After update to highcharts.js today we get Highcharts.chart is not a constructor - Stack Overflow](https://stackoverflow.com/questions/76111359/after-update-to-highcharts-js-today-we-get-highcharts-chart-is-not-a-constructor)

I changed the code like this:

vrishabkakade@freedompi:/etc/weewx/skins/Belchertown/js $ ls -lrat

total 304  
-rw-rw-r-- 1 weewx weewx 765 Apr 13 11:49 responsive-menu.js  
-rw-rw-r-- 1 weewx weewx 14 Apr 13 11:49 index.html  
drwxr-sr-x 11 weewx weewx 4096 Apr 13 14:12 ..  
-rw-r--r-- 1 root weewx 143973 Apr 13 14:51 belchertown.js.tmpl.orig  
drwxr-sr-x 2 weewx weewx 4096 Apr 13 14:51 .  
-rw-rw-r-- 1 weewx weewx 143973 Apr 13 14:58 belchertown.js.tmpl

vrishabkakade@freedompi:/etc/weewx/skins/Belchertown/js $ vi belchertown.js.tmpl

Line 2895 comment and duplicate – remove new word as per the solution

*// Finally all options are done, now show the chart*

*//var chart = new Highcharts.chart(options);*

var chart = Highcharts.chart(options);

### 💿 Setup SMB Server on the Raspberry Pi

[How to Setup a Raspberry Pi Samba Server - Pi My Life Up](https://pimylifeup.com/raspberry-pi-samba/)

I’m setting up a SMB server on Raspberry Pi to access the database file from my laptop which is Windows.

The first thing that we must do before we setup a SMB/CIFS share on our Raspberry Pi is to make sure everything is up to date.

We can update the package list and all our packages by running the following two commands.

sudo apt-get update

sudo apt-get upgrade

Now that we have our Raspbian operating system entirely up to date, we can now proceed on to installing the Samba software to our Raspberry Pi.

We can install the packages that we require to setup Samba by running the following command.

sudo apt-get install samba samba-common-bin

Now we can share this folder using the Samba software. To do this, we need to modify the samba config file.

The “smb.conf” configuration file is where you will store all your settings for your shares.

We can begin modifying the config file by running the command below.

sudo vi /etc/samba/smb.conf

[freedompishare]  
path = /var/lib/weewx  
**writeable**=Yes  
create **mask**=0777  
directory **mask**=0777  
**public**=no

Next, we need to set up a user for our Samba share on the Raspberry Pi. Without it, we won’t be able to make a connection to the shared network drive.

vrishabkakade@freedompi:/etc/weewx/skins/Belchertown $ sudo smbpasswd -a weewx

Finally, before we connect to our Raspberry Pi Samba share, we need to restart the samba service so that it loads in our configuration changes.

sudo systemctl restart smbd

### 🪈 MQTT and MQTT Websockets (optional)

Source: [How to setup your own MQTT Broker – O'Brien Labs (obrienlabs.net)](https://obrienlabs.net/how-to-setup-your-own-mqtt-broker/)

From the Author

I wrote this MQTT tutorial to help me out in the future, but hopefully it helps someone else along the way!

For the last few years I’ve been running a [custom weather website](https://belchertownweather.com/). This website, in conjunction with [weewx](http://weewx.com/" \t "_blank), allowed me to have a website which updated itself every 10 seconds. But this bothered me. **10 seconds was far too slow for my liking!**

Earlier this year (2018) I started using [Home Assistant](http://hass.io/) for home automation (goodbye old unreliable cloud-based automation!) and they opened me up to MQTT. It was great to be able to get data from tiny Arduino sensors around the house – but I knew I could do more with it. That’s when I saw an [MQTT extension available for weewx](https://github.com/weewx/weewx/wiki/mqtt). I knew it was time for a [website upgrade](https://github.com/poblabs/weewx-belchertown)!

**The result was a true real time auto updating website with no delay!** Every time my weather station sends an update from the backyard (every 2.5 seconds), that data is immediately read by weewx which archives the data, runs some QC checks on it for accuracy, then publishes it to MQTT. Visitors on my website auto-subscribe to the MQTT topic through websockets and JavaScript updates the data on the webpage within milliseconds. It’s really cool!

If you’re not familiar with MQTT, it’s a machine-to-machine internet of things (IoT) communication protocol. Initially designed as a lightweight publish/subscribe method useful for those devices in remote locations with limited internet connectivity. It even works great for Arduino or NodeMCU temperature sensors around the house. The device that needs to send data would publish to a topic, and the device that needs to receive that data would subscribe to that topic. Topic names are arbitrary, but they should make sense. For example a topic could be weather/weewx/loop. This could mean it’s the weather parent category, the weewx software, and the loop function. Then you could have weather/weewx/archive for archive data, weather/rain\_bucket/current if you had a rain bucket that can talk MQTT. Whatever you want!

I have weewx configured to publish weather loop data to the topic weather/weewx/loop, and my website is configured to subscribe on that topic.

Due to the high nature that weewx publishes weather data (currently my loop is at **2.5 seconds**), I couldn’t use a free MQTT broker (or server), and I didn’t want to pay for access to one. Some free ones will handle the frequent data, but offer no uptime reliability, so I decided to install my own broker.

* **Total time to setup: 5 – 30 minutes.**

This tutorial was created in 2018 using Ubuntu 18.04, so some things may be different after I write this or if you use another operating system.

You can run MQTT on a Raspberry Pi, but I recommend running MQTT on a cloud server because it’s always available, fast and easy.

Running this on the virtual server

#### Install Mosquitto

First install Mosquitto, which is the name of the MQTT software.

[weewx@cloud009 ~]$ sudo apt update

[weewx@cloud009 ~]$ sudo apt-get install mosquitto mosquitto-clients

#### Setup websockets

If you plan on using your MQTT Broker for a website, like the [Belchertown weewx skin](https://github.com/poblabs/weewx-belchertown), then you need to enable websockets.

Let’s create a custom configuration file that we’ll add this – and other items – to for Mosquitto’s config. Run sudo nano /etc/mosquitto/conf.d/myconfig.conf and update it with the below:

[weewx@cloud009 ~]$ sudo vi /etc/mosquitto/conf.d/myconfig.con

persistence false  
  
# mqtt  
listener 1883  
protocol mqtt  
  
# websockets  
listener 9001  
protocol websockets

Make sure you have no empty spaces at the end of those lines or Mosquitto may give you an error.

Restart Mosquitto with sudo service mosquitto restart and you should now have a working MQTT server on port 1883 and websockets on port 9001!

[weewx@cloud009 ~]$ sudo service mosquitto restart

#### Create a user and access control

I locked down my broker so that only those clients who know the password can publish to a topic. You can get super granular here where certain usernames can publish to certain topics only. For my sake I only have 1 user who can publish. All other users who connect to the broker are considered anonymous and can only subscribe. Create a password for publishing with:

[weewx@cloud009 ~]$ sudo mosqusudo mosquitto\_passwd -c /etc/mosquitto/passwd weewx

Next is to create an MQTT ACL (access control list) so that anonymous users are read only, but the weewx system can read and write to the weather topic. Run sudo nano /etc/mosquitto/acl and enter in:

[weewx@cloud009 ~]$ sudo vi /etc/mosquitto/acl

# Allow anonymous access to the sys  
topic read $SYS/#  
  
# Allow anonymous to read weather  
topic read weather/#  
  
# weewx readwrite to the loop  
user weewx  
topic weather/#

#### Add to the custom broker configuration

Now let’s add the authentication and access control to the custom configuration file. Run sudo nano /etc/mosquitto/conf.d/myconfig.conf and enter in:

[weewx@cloud009 ~]$ sudo vi /etc/mosquitto/conf.d/myconfig.conf

allow\_anonymous **true**  
password\_file /etc/mosquitto/passwd  
  
acl\_file /etc/mosquitto/acl

Save your file and run mosquitto with mosquitto -c /etc/mosquitto/mosquitto.conf and with another SSH client, log into your server and check that the MQTT ports are open. Run this command sudo netstat -tulpn | grep 1883 and you should see port 1883 open. Repeat with port 9001 to verify websockets are open. It should look something like:

tcp 0 0 127.0.0.1:1883 0.0.0.0:\* LISTEN 973/mosquitto

If it’s open like above then open 2 more SSH connections to your server to test publish and subscribe.

[weewx@cloud009 ~]$ sudo mosquitto -c /etc/mosquitto/mosquitto.conf

[weewx@cloud009 ~]$ sudo netstat -tulpn | grep 1883

tcp 0 0 127.0.0.1:1883 0.0.0.0:\* LISTEN 114850/mosquitto  
tcp6 0 0 ::1:1883 :::\* LISTEN 114850/mosquitto

Session 1: run this command to subscribe to the weather topic.

mosquitto\_sub -h localhost -t weather/#

The # means you want to listen on everything underneath weather. For example weather/topic1, weather/topic2, weather/topic3, etc.

Note: Only use # when troubleshooting. You shouldn’t setup your website or application to publish or subscribe to # in a normal situation.

Session 2: try to publish using this command:

mosquitto\_pub -h localhost -t "weather/test" -m "hello world"`

[weewx@cloud009 ~]$ mosquitto\_mosquitto\_pub -h localhost -t "weather/test" -m "hello world"

[weewx@cloud009 ~]$ mosquitto\_sub -h localhost -t weather/#

**hello world**

This command does not use any authentication so **it should fail**! Your mosquitto\_sub window should not show anything. If you do not see anything, so far so good!

Now go back to SSH #2 (with the mosquitto\_pub) and run this command which has authentication:

mosquitto\_pub -h localhost -t "weather/test" -m "hello world. this is to the weather topic with authentication" -u "<your username from above>" -P "<your password you created>"

[weewx@cloud009 ~]$ mosquitto\_mosquitto\_pub -h localhost -t "weather/test" -m "hello world. this is to the weather topic with authentication" -u "weewx" -P "\*\*\*\*"

[weewx@cloud009 ~]$ mosquitto\_sub -h localhost -t weather/#

hello world  
hello world. **this** **is** **to** the weather topic **with** authentication

You should see something in your mosquitto\_sub window now! If you do, great! If not, back up and try everything again. Sometimes Mosquitto is fussy and requires a full reboot. You can also check the Mosquitto log file at /var/log/mosquitto/mosquitto.log

So if you’ve made it this far you have a working MQTT broker with authentication and websockets!

#### Setup LetsEncrypt SSL certificate (optional)

Using the SSL cert setup with the website

#### Add your SSL cert to MQTT config

Update your custom MQTT config file and add the new SSL certificates. Run sudo nano /etc/mosquitto/conf.d/myconfig.conf and update it with the below:

[weewx@cloud009 ~]$ sudo vi /etc/mosquitto/conf.d/myconfig.conf

allow\_anonymous true  
password\_file /etc/mosquitto/passwd  
  
  
acl\_file /etc/mosquitto/acl  
  
persistence false  
  
# mqtt  
listener 1883  
listener 8883  
certfile /etc/mosquitto/certs/cert.pem  
cafile /etc/mosquitto/certs/chain.pem  
keyfile /etc/mosquitto/certs/privkey.pem  
protocol mqtt  
  
# websockets  
listener 9001  
certfile /etc/mosquitto/certs/cert.pem  
cafile /etc/mosquitto/certs/chain.pem  
keyfile /etc/mosquitto/certs/privkey.pem

[weewx@cloud009 ~]$ sudo ls -lrat /etc/letsencrypt/archive/bettaforecast.in

total 24  
-rw------- 1 root root 1704 Apr 12 16:35 privkey1.pem  
-rw-r--r-- 1 root root 3595 Apr 12 16:35 fullchain1.pem  
-rw-r--r-- 1 root root 1826 Apr 12 16:35 chain1.pem  
-rw-r--r-- 1 root root 1769 Apr 12 16:35 cert1.pem  
drwx------ 3 root root 4096 Apr 12 16:35 ..  
drwxr-xr-x 2 root root 4096 Apr 12 16:35 .

I get the below error with the above permissions

1713070124: Error: Unable to load CA certificates. Check cafile "/etc/letsencrypt/live/bettaforecast.in/chain.pem".  
1713070124: OpenSSL Error[0]: error:8000000D:system library::Permission denied  
1713070124: OpenSSL Error[1]: error:10080002:BIO routines::system **lib**  
1713070124: OpenSSL Error[2]: error:05880002:x509 certificate routines::system **lib**

Copy the certificates to a new location and change permissions there so that we don’t affect the Apache Letsencrypt certificates.

[root@cloud009 ~]$ cat /etc/mosqu/etc/mosquitto/certs/copy\_ssl\_certs\_mqtt.sh

#!/bin/bash  
SHELL=/bin/bash  
export PATH=/usr/local/sbin:/usr/local/bin:/usr/sbin:/usr/bin:/sbin:/bin:/usr/games:/usr/local/games:/snap/bin:$PATH  
cp /etc/letsencrypt/live/bettaforecast.**in**/privkey.pem /etc/mosquitto/certs  
cp /etc/letsencrypt/live/bettaforecast.**in**/fullchain.pem /etc/mosquitto/certs  
cp /etc/letsencrypt/live/bettaforecast.**in**/chain.pem /etc/mosquitto/certs  
cp /etc/letsencrypt/live/bettaforecast.**in**/cert.pem /etc/mosquitto/certs

Put it in the crontab so the script can run everyday.

[root@cloud009 ~]$ crontab -l

52 \* \* \* \* cd /etc/mosquitto/certs && /**usr**/bin/sh /etc/mosquitto/certs/copy\_ssl\_certs\_mqtt.sh >> /etc/mosquitto/certs/copy\_ssl\_certs\_mqtt.**log** 2>&1  
0 0 \* \* 0 /home/weewx/backup\_scripts/backup\_weewx.sh

Restart your mosquitto server with sudo service mosquitto restart and check that the ports are open with sudo netstat -tulpn | grep -E '8883|9001'. You should see something similar to:

[weewx@cloud009 /etc/mosquitto/certs]$ sudo service mosquitto restart

[weewx@cloud009 /etc/mosquitto/certs]$ sudo netstat -tulpn | grep -E '8883|9001'

tcp 0 0 0.0.0.0:8883 0.0.0.0:\* LISTEN 123262/mosquitto  
tcp6 0 0 :::9001 :::\* LISTEN 123262/mosquitto  
tcp6 0 0 :::8883 :::\* LISTEN 123262/mosquito

#### Install Mosquito on the Raspberry Pi

We need Mosquito installed on the Raspberry Pi as well since the messages get sent in real-time from the Raspberry Pi to the web server.

weewx@freedompi:~$ sudo apt update

weewx@freedompi:~$ sudo apt-get install mosquitto mosquitto-clients

weewx@freedompi:~$ sudo service mosquitto start

Test it

mosquitto\_pub -h bettaforecast.in -t "weather/test" -m "hello world. this is to the weather topic with authentication 2" -u "weewx" -P "\*\*\*"

#### Customize the Graphs

Source: [Belchertown Charts Documentation · poblabs/weewx-belchertown Wiki (github.com)](https://github.com/poblabs/weewx-belchertown/wiki/Belchertown-Charts-Documentation#zindex)

The document is very well written and I have made a lot of customizations. Refer to the below file

weewx@freedompi:/etc/weewx/skins/Belchertown$ ls -lrat graphs.conf

-rw-r--r-- 1 weewx weewx 23308 Apr 17 09:40 graphs.conf

vince's profile photo

### **vince**

unread,

Mar 27, 2021, 9:21:54 PM







to weewx-user

> server\_url = mqtt://tph06784:xxxx@localhost:1883

This is becoming a FAQ.

Do not use 'localhost'.  Use the fully qualified domain name of the MQTT broker host or its IP address.

[MQTT for Belchertown skin (google.com)](https://groups.google.com/g/weewx-user/c/V5QYIeUNNJ4)

SCRIPT TO AUTOMATE COPYING OF CERTS FOR MQTT

Source certs

[weewx@cloud009 ~]$ sudo ls -lrat /etc/letsencrypt/live/bettaforecast.in

total 12

lrwxrwxrwx 1 root root 43 Apr 12 16:35 privkey.pem -> ../../archive/bettaforecast.in/privkey1.pem

lrwxrwxrwx 1 root root 45 Apr 12 16:35 fullchain.pem -> ../../archive/bettaforecast.in/fullchain1.pem

lrwxrwxrwx 1 root root 41 Apr 12 16:35 chain.pem -> ../../archive/bettaforecast.in/chain1.pem

lrwxrwxrwx 1 root root 40 Apr 12 16:35 cert.pem -> ../../archive/bettaforecast.in/cert1.pem

drwx------ 3 root root 4096 Apr 12 16:35 ..

drwxr-xr-x 2 root root 4096 Apr 12 16:35 .

-rw-r--r-- 1 root root 692 Apr 12 16:35 README

MQTT Certs

[weewx@cloud009 ~]$ ls -lrat /etc/mosquitto/certs

total 28

-rw-r--r-- 1 weewx weewx 130 Nov 19 23:39 README

drwxr-xr-x 5 root root 4096 Apr 14 08:43 ..

-rwxr-xr-x 1 weewx weewx 1704 Apr 14 10:24 privkey.pem

-rwxr-xr-- 1 weewx weewx 3595 Apr 14 10:24 fullchain.pem

-rwxr-xr-- 1 weewx weewx 1826 Apr 14 10:24 chain.pem

-rwxr-xr-- 1 weewx weewx 1769 Apr 14 10:24 cert.pem

drwxr-xr-x 2 weewx weewx 4096 Apr 14 22:38 .

[weewx@cloud009 ~]$ cd /etc/mosquitto/certs

[weewx@cloud009 /etc/mosquitto/certs]$ vi copy\_ssl\_certs\_mqtt.sh

#!/bin/bash

SHELL=/bin/bash

export PATH=/usr/local/sbin:/usr/local/bin:/usr/sbin:/usr/bin:/sbin:/bin:/usr/games:/usr/local/games:/snap/bin:$PATH

cp /etc/letsencrypt/live/bettaforecast.in/privkey.pem /etc/mosquitto/certs

cp /etc/letsencrypt/live/bettaforecast.in/fullchain.pem /etc/mosquitto/certs

cp /etc/letsencrypt/live/bettaforecast.in/chain.pem /etc/mosquitto/certs

cp /etc/letsencrypt/live/bettaforecast.in/cert.pem /etc/mosquitto/certs

[weewx@cloud009 /etc/mosquitto/certs]$ chmod 755 copy\_ssl\_certs\_mqtt.sh

[root@cloud009 ~]$ crontab -e

# m h dom mon dow command

52 \* \* \* \* cd /etc/mosquitto/certs && /usr/bin/sh /etc/mosquitto/certs/copy\_ssl\_certs\_mqtt.sh >> /etc/mosquitto/certs/copy\_ssl\_certs\_mqtt.log 2>&1

In my case I had to restart cron. No jobs were running from any user.

[root@cloud009 /etc/mosquitto/certs]$ sudo systemctl restart cron

[mqtt · weewx/weewx Wiki (github.com)](https://github.com/weewx/weewx/wiki/mqtt)

weewx@freedompi:~$ sudo pip3 install paho-mqtt==1.6.1

weewx@freedompi:~$ wget -O weewx-mqtt.zip <https://github.com/matthewwall/weewx-mqtt/archive/master.zip>

weewx@freedompi:~$ sudo weectl extension install weewx-mqtt.zip

Copy the certs to the raspberry pi as well

weewx@bettaforecastpi:/tmp/certs $ ls -lrat /etc/mosquitto/certs

total 28

drwxr-xr-x 5 root root 4096 May 9 20:05 ..

-rwxr-xr-x 1 weewx weewx 1826 May 9 20:16 chain.pem

-rwxr-xr-x 1 weewx weewx 1704 May 9 20:16 privkey.pem

-rwxr-xr-x 1 weewx weewx 130 May 9 20:16 README

-rwxr-xr-x 1 weewx weewx 3595 May 9 20:16 fullchain.pem

-rwxr-xr-x 1 weewx weewx 1769 May 9 20:16 cert.pem

drwxr-xr-x 2 root root 4096 May 9 20:17 .

## Windy

[matthewwall/weewx-windy: uploader for windy.com (github.com)](https://github.com/matthewwall/weewx-windy)

weewx@bettaforecastpi:/var/lib/weewx $ cd /tmp

weewx@bettaforecastpi:/tmp $ wget -O weewx-windy.zip <https://github.com/matthewwall/weewx-windy/archive/master.zip>

weewx@bettaforecastpi:/tmp $ sudo weectl extension install weewx-windy.zip

SITEMAP

<https://www.youtube.com/watch?v=HDJAyf007sI>

[clusterednetworks/sitemap-generator-cron: A script to be run as a cronjob using sitemap-generator-cli (github.com)](https://github.com/clusterednetworks/sitemap-generator-cron)

[lgraubner/sitemap-generator-cli: Creates an XML-Sitemap by crawling a given site. (github.com)](https://github.com/lgraubner/sitemap-generator-cli?tab=readme-ov-file)

I landed up using this my correcting the script myself

[poblabs/sitemap-generator (github.com)](https://github.com/poblabs/sitemap-generator)

## **Backup**[**¶**](https://weewx.com/docs/5.0/usersguide/backup/#backup)

To back up a WeeWX installation, you will need to make a copy of

* the configuration information (**weewx.conf**),
* skins and templates,
* custom code, and
* the WeeWX database.

The location of these items depends on how you installed WeeWX.

Debian

| **Item** | **Location** |
| --- | --- |
| Configuration | **/etc/weewx/weewx.conf** |
| Skins | **/etc/weewx/skins** |
| Custom code | **/etc/weewx/bin/user** |
| Database | **/var/lib/weewx/weewx.sdb** |

It is not necessary to back up the generated images, HTML files, or NOAA reports, because WeeWX can easily regenerate them.

It is also not necessary to back up the WeeWX code, because it can be installed again. However, it doesn't hurt to do so.

**Note**

For a SQLite configuration, do not make the copy of the database file while in the middle of a transaction! Schedule the backup for immediately after an archive record is written, and then make sure the backup completes before the next archive record arrives. Alternatively, stop WeeWX, perform the backup, then start WeeWX.

**Note**

For a MySQL/MariaDB configuration, save a dump of the archive database.

vrishabkakade@freedompi:~/backup\_scripts $ cat backup\_weewx.sh

cd /mnt/backup

sudo touch weewx\_bkp\_`hostname`\_`date +%Y%m%d`.log

sudo chmod 777 weewx\_bkp\_`hostname`\_`date +%Y%m%d`.log

sudo tar -zcvf weewx\_bkp\_`hostname`\_`date +%Y%m%d`.tar /var/lib/weewx /var/www/html/weewx /etc/weewx /etc/apache2 /etc/mosquitto /home/vrishabkakade >> weewx\_bkp\_`hostname`\_`date +%Y%m%d`.log

if [ `sudo echo $?` -eq 0 ]

then

sudo echo "Backup Success" >> weewx\_bkp\_`hostname`\_`date +%Y%m%d`.log

else

sudo echo "Backup failed" >> weewx\_bkp\_`hostname`\_`date +%Y%m%d`.log

fi

vrishabkakade@freedompi:~ $ crontab -l

0 0 \* \* 0 /home/vrishabkakade/backup\_scripts/backup\_weewx.sh

ON WEB SERVER

[weewx@cloud009 ~]$ cd /mnt

[weewx@cloud009 /mnt]$ ls

[weewx@cloud009 /mnt]$ sudo mkdir backup

[sudo] password for weewx:

[weewx@cloud009 /mnt]$ mkdir backup scripts

mkdir: cannot create directory ‘backup’: File exists

mkdir: cannot create directory ‘scripts’: Permission denied

[weewx@cloud009 /mnt]$ mkdir back^C scripts

[weewx@cloud009 /mnt]$ cd

[weewx@cloud009 ~]$ mkdir backup\_scripts

[weewx@cloud009 ~]$ cd backup\_scripts/

[weewx@cloud009 ~/backup\_scripts]$ vi backup\_weewx.sh

[weewx@cloud009 ~/backup\_scripts]$

[weewx@cloud009 ~/backup\_scripts]$

[weewx@cloud009 ~/backup\_scripts]$ chmod +x backup\_weewx.sh

[weewx@cloud009 ~/backup\_scripts]$ cat backup\_weewx.sh

cd /mnt/backup

sudo touch weewx\_bkp\_`hostname`\_`date +%Y%m%d`.log

sudo chmod 777 weewx\_bkp\_`hostname`\_`date +%Y%m%d`.log

sudo tar -zcvf weewx\_bkp\_`hostname`\_`date +%Y%m%d`.tar /var/www /etc/apache2 /home/weewx /etc/letsencrypt >> weewx\_bkp\_`hostname`\_`date +%Y%m%d`.log

if [ `sudo echo $?` -eq 0 ]

then

sudo echo "Backup Success" >> weewx\_bkp\_`hostname`\_`date +%Y%m%d`.log

else

sudo echo "Backup failed" >> weewx\_bkp\_`hostname`\_`date +%Y%m%d`.log

fi

I have to run it as root as it keeps prompting for sudo password otherwise

[root@cloud009 ~]$ crontab -l

52 \* \* \* \* cd /etc/mosquitto/certs && /usr/bin/sh /etc/mosquitto/certs/copy\_ssl\_certs\_mqtt.sh >> /etc/mosquitto/certs/copy\_ssl\_certs\_mqtt.log 2>&1

0 0 \* \* 0 /home/weewx/backup\_scripts/backup\_weewx.sh

MQTT Won’t work on Firefox

<https://support.mozilla.org/en-US/questions/1324001>

Error:

the connection to wss:bettaforecast.in:9001 mqtt was interrupted while the page was loading.

Your page's behavior seems to match a pattern of problems with Firefox attempting to make an SSL connection to MQTT servers via HTTP/2. Users can disable HTTP/2 for Websockets --

(1) In a new tab, type or paste **about:config** in the address bar and press Enter/Return. Click the button accepting the risk.

(2) In the search box in the page, type or paste **websockets** and pause while the list is filtered


(3) Double-click the **network.http.spdy.websockets** preference to switch the value from true to false (switches Firefox from using HTTP/2 to HTTP/1.1 for WebSockets)

-- but that isn't something the server could dictate to Firefox users.

* <https://github.com/eclipse/paho.mqtt.javascript/issues/231>
* <https://github.com/eclipse/mosquitto/issues/1211>

What makes this even stranger is that the Websocket connection the page is making to the radar server is working just fine with the standard setting. ??

[Read this answer in context](https://support.mozilla.org/en-US/questions/1324001#answer-1388648) **👍 1**



SIZE OF HIDDEN FILES - du -sh $(ls -A)

[bash - How to get size of hidden files with "du" - Stack Overflow](https://stackoverflow.com/questions/67836594/how-to-get-size-of-hidden-files-with-du)

[Update process hangs during a fresh installation of Raspberry Pi OS - Raspberry Pi Forums](https://forums.raspberrypi.com/viewtopic.php?t=359240)

There’s an issue where the processes can hang and run out of memory as the RAM on the pi zero is just 512M and swap by default is 100M. Increase the swap to 1024M by editing the below file

weewx@bettaforecastpi:~ $ sudo vi /etc/dphys-swapfile

change CONF\_SWAPSIZE=100 to 1024